DEVLINK-HEALTH(8)

NAME
devlink-health - devlink health reporting and recovery

SYNOPSIS

devlink [ OPTIONS ] health { COMMAND | help }

OPTIONS := { -V[ersion] }
devlink health show [ { DEV | DEV/PORT_INDEX } reporter REPORTER ]
devlink health recover { DEV | DEV/PORT_INDEX } reporter REPORTER
devlink health diagnose { DEV | DEV/PORT_INDEX } reporter REPORTER
devlink health dump show { DEV | DEV/PORT_INDEX } reporter REPORTER
devlink health test { DEV | DEV/PORT_INDEX } reporter REPORTER
devlink health dump clear { DEV | DEV/PORT_INDEX } reporter REPORTER
devlink health set { DEV | DEV/PORT_INDEX } reporter REPORTER [ grace_period MSEC ] [ auto_recover { true | false } ] [ auto_dump { true | false } ]
devlink health help

DESCRIPTION

  devlink health show - Show status and configuration on all supported reporters.
Displays info about reporters registered on devlink devices and ports.

DEV - specifies the devlink device.
DEV/PORT_INDEX - specifies the devlink port.

REPORTER - specifies the reporter's name registered on specified devlink device or port.

  devlink health recover - Initiate a recovery operation on a reporter.
This action performs a recovery and increases the recoveries counter on success.

DEV - specifies the devlink device.
DEV/PORT_INDEX - specifies the devlink port.

REPORTER - specifies the reporter's name registered on specified devlink device or port.

  devlink health diagnose - Retrieve diagnostics data on a reporter.

DEV - specifies the devlink device.
DEV/PORT_INDEX - specifies the devlink port.

REPORTER - specifies the reporter's name registered on specified devlink device or port.

  devlink health test - Trigger a test event on a reporter.

DEV - specifies the devlink device.

REPORTER - specifies the reporter's name registered on the devlink device.

  devlink health dump show - Display the last saved dump.
devlink health saves a single dump per reporter. If an dump is
not already stored by the Devlink, this command will generate a new
dump. The dump can be generated either automatically when a
reporter reports on an error or manually at the user's request.

DEV - specifies the devlink device.
DEV/PORT_INDEX - specifies the devlink port.

REPORTER - specifies the reporter's name registered on specified devlink device or port.

  devlink health dump clear - Delete the saved dump.
Deleting the saved dump enables a generation of a new dump on
the next "devlink health dump show" command.

DEV - specifies the devlink device.
DEV/PORT_INDEX - specifies the devlink port.

REPORTER - specifies the reporter's name registered on specified devlink device or port.

  devlink health set - Configure health reporter.
Please note that some params are not supported on a reporter which doesn't support a recovery or dump method.

DEV - specifies the devlink device.
DEV/PORT_INDEX - specifies the devlink port.

REPORTER - specifies the reporter's name registered on specified devlink device or port.

grace_period MSEC
    Time interval between consecutive auto recoveries.

auto_recover { true | false }
    Indicates whether the devlink should execute automatic recover on error.

auto_dump { true | false }
    Indicates whether the devlink should execute automatic dump on error.

EXAMPLES

devlink health show
    List status and configuration of available reporters on devices and ports.

devlink health show pci/0000:00:09.0/1 reporter tx
    List status and configuration of tx reporter registered on port on pci/0000:00:09.0/1

devlink health recover pci/0000:00:09.0 reporter fw_fatal
    Initiate recovery on fw_fatal reporter registered on device on pci/0000:00:09.0.

devlink health recover pci/0000:00:09.0/1 reporter tx
    Initiate recovery on tx reporter registered on port on pci/0000:00:09.0/1.

devlink health diagnose pci/0000:00:09.0 reporter fw
    List diagnostics data on the specified device and reporter.

devlink health dump show pci/0000:00:09.0/1 reporter tx
    Display the last saved dump on the specified port and reporter.

devlink health dump clear pci/0000:00:09.0/1 reporter tx
    Delete saved dump on the specified port and reporter.

devlink health set pci/0000:00:09.0 reporter fw_fatal grace_period 3500
    Set time interval between auto recoveries to minimum of 3500 msec on the specified device and reporter.

devlink health set pci/0000:00:09.0/1 reporter tx grace_period 3500
    Set time interval between auto recoveries to minimum of 3500 msec on the specified port and reporter.

devlink health set pci/0000:00:09.0 reporter fw_fatal auto_recover false
    Turn off auto recovery on the specified device and reporter.

SEE ALSO
devlink(8), devlink-dev(8), devlink-port(8), devlink-param(8), devlink-region(8),

AUTHOR
Aya Levin <ayal@mellanox.com>