NM-SETTINGS-NMCLI(5)

NAME
nm-settings-nmcli - Description of settings and properties of NetworkManager connection profiles for nmcli

DESCRIPTION

NetworkManager is based on a concept of connection profiles, sometimes referred to as connections only. These connection profiles contain a network configuration. When NetworkManager activates a connection profile on a network device the configuration will be applied and an active network connection will be established. Users are free to create as many connection profiles as they see fit. Thus they are flexible in having various network configurations for different networking needs.

NetworkManager provides an API for configuring connection profiles, for activating them to configure the network, and inspecting the current network configuration. The command line tool nmcli is a client application to NetworkManager that uses this API. See nmcli(1) for details.

With commands like nmcli connection add, nmcli connection modify and nmcli connection show, connection profiles can be created, modified and inspected. A profile consists of properties. On D-Bus this follows the format as described by nm-settings-dbus(5), while this manual page describes the settings format how they are expected by nmcli.

The settings and properties shown in tables below list all available connection configuration options. However, note that not all settings are applicable to all connection types. nmcli connection editor has also a built-in describe command that can display description of particular settings and properties of this page.

The setting and property can be abbreviated provided they are unique. The list below also shows aliases that can be used unqualified instead of the full name. For example connection.interface-name and ifname refer to the same property.

  connection setting

General Connection Profile Settings.

Properties:

connection.auth-retries
    The number of retries for the authentication. Zero means to try indefinitely; -1 means to use a global default. If the global default is not set, the authentication retries for 3 times before failing the connection.

    Currently, this only applies to 802-1x authentication.

    Format: int32

connection.autoconnect
    Alias: autoconnect

    Whether or not the connection should be automatically connected by NetworkManager when the resources for the connection are available. TRUE to automatically activate the connection, FALSE to require manual intervention to activate the connection.

    Autoconnect happens when the circumstances are suitable. That means for example that the device is currently managed and not active. Autoconnect thus never replaces or competes with an already active profile.

    Note that autoconnect is not implemented for VPN profiles. See "secondaries" as an alternative to automatically connect VPN profiles.

    If multiple profiles are ready to autoconnect on the same device, the one with the better "connection.autoconnect-priority" is chosen. If the priorities are equal, then the most recently connected profile is activated. If the profiles were not connected earlier or their "connection.timestamp" is identical, the choice is undefined.

    Depending on "connection.multi-connect", a profile can (auto)connect only once at a time or multiple times.

    Format: boolean

connection.autoconnect-priority
    The autoconnect priority in range -999 to 999. If the connection is set to autoconnect, connections with higher priority will be preferred. The higher number means higher priority. Defaults to 0. Note that this property only matters if there are more than one candidate profile to select for autoconnect. In case of equal priority, the profile used most recently is chosen.

    Format: int32

connection.autoconnect-retries
    The number of times a connection should be tried when autoactivating before giving up. Zero means forever, -1 means the global default (4 times if not overridden). Setting this to 1 means to try activation only once before blocking autoconnect. Note that after a timeout, NetworkManager will try to autoconnect again.

    Format: int32

connection.autoconnect-slaves
    Whether or not slaves of this connection should be automatically brought up when NetworkManager activates this connection. This only has a real effect for master connections. The properties "autoconnect", "autoconnect-priority" and "autoconnect-retries" are unrelated to this setting. The permitted values are: 0: leave slave connections untouched, 1: activate all the slave connections with this connection, -1: default. If -1 (default) is set, global connection.autoconnect-slaves is read to determine the real value. If it is default as well, this fallbacks to 0.

    Format: NMSettingConnectionAutoconnectSlaves (int32)

connection.dns-over-tls
    Whether DNSOverTls (dns-over-tls) is enabled for the connection. DNSOverTls is a technology which uses TLS to encrypt dns traffic.

    The permitted values are: "yes" (2) use DNSOverTls and disabled fallback, "opportunistic" (1) use DNSOverTls but allow fallback to unencrypted resolution, "no" (0) don't ever use DNSOverTls. If unspecified "default" depends on the plugin used. Systemd-resolved uses global setting.

    This feature requires a plugin which supports DNSOverTls. Otherwise, the setting has no effect. One such plugin is dns-systemd-resolved.

    Format: int32

connection.gateway-ping-timeout
    If greater than zero, delay success of IP addressing until either the timeout is reached, or an IP gateway replies to a ping.

    Format: uint32

connection.id
    Alias: con-name

    A human readable unique identifier for the connection, like "Work Wi-Fi" or "T-Mobile 3G".

    Format: string

connection.interface-name
    Alias: ifname

    The name of the network interface this connection is bound to. If not set, then the connection can be attached to any interface of the appropriate type (subject to restrictions imposed by other settings).

    For software devices this specifies the name of the created device.

    For connection types where interface names cannot easily be made persistent (e.g. mobile broadband or USB Ethernet), this property should not be used. Setting this property restricts the interfaces a connection can be used with, and if interface names change or are reordered the connection may be applied to the wrong interface.

    Format: string

connection.lldp
    Whether LLDP is enabled for the connection.

    Format: int32

connection.llmnr
    Whether Link-Local Multicast Name Resolution (LLMNR) is enabled for the connection. LLMNR is a protocol based on the Domain Name System (DNS) packet format that allows both IPv4 and IPv6 hosts to perform name resolution for hosts on the same local link.

    The permitted values are: "yes" (2) register hostname and resolving for the connection, "no" (0) disable LLMNR for the interface, "resolve" (1) do not register hostname but allow resolving of LLMNR host names If unspecified, "default" ultimately depends on the DNS plugin (which for systemd-resolved currently means "yes").

    This feature requires a plugin which supports LLMNR. Otherwise, the setting has no effect. One such plugin is dns-systemd-resolved.

    Format: int32

connection.master
    Alias: master

    Interface name of the master device or UUID of the master connection.

    Format: string

connection.mdns
    Whether mDNS is enabled for the connection.

    The permitted values are: "yes" (2) register hostname and resolving for the connection, "no" (0) disable mDNS for the interface, "resolve" (1) do not register hostname but allow resolving of mDNS host names and "default" (-1) to allow lookup of a global default in NetworkManager.conf. If unspecified, "default" ultimately depends on the DNS plugin (which for systemd-resolved currently means "no").

    This feature requires a plugin which supports mDNS. Otherwise, the setting has no effect. One such plugin is dns-systemd-resolved.

    Format: int32

connection.metered
    Whether the connection is metered.

    When updating this property on a currently activated connection, the change takes effect immediately.

    Format: NMMetered (int32)

connection.mptcp-flags
    Whether to configure MPTCP endpoints and the address flags. If MPTCP is enabled in NetworkManager, it will configure the addresses of the interface as MPTCP endpoints. Note that IPv4 loopback addresses (127.0.0.0/8), IPv4 link local addresses (169.254.0.0/16), the IPv6 loopback address (::1), IPv6 link local addresses (fe80::/10), IPv6 unique local addresses (ULA, fc00::/7) and IPv6 privacy extension addresses (rfc3041, ipv6.ip6-privacy) will be excluded from being configured as endpoints.

    If "disabled" (0x1), MPTCP handling for the interface is disabled and no endpoints are registered.

    The "enabled" (0x2) flag means that MPTCP handling is enabled. This flag can also be implied from the presence of other flags.

    Even when enabled, MPTCP handling will by default still be disabled unless "/proc/sys/net/mptcp/enabled" sysctl is on. NetworkManager does not change the sysctl and this is up to the administrator or distribution. To configure endpoints even if the sysctl is disabled, "also-without-sysctl" (0x4) flag can be used. In that case, NetworkManager doesn't look at the sysctl and configures endpoints regardless.

    Even when enabled, NetworkManager will only configure MPTCP endpoints for a certain address family, if there is a unicast default route (0.0.0.0/0 or ::/0) in the main routing table. The flag "also-without-default-route" (0x8) can override that.

    When MPTCP handling is enabled then endpoints are configured with the specified address flags "signal" (0x10), "subflow" (0x20), "backup" (0x40), "fullmesh" (0x80). See ip-mptcp(8) manual for additional information about the flags.

    If the flags are zero (0x0), the global connection default from NetworkManager.conf is honored. If still unspecified, the fallback is "enabled,subflow". Note that this means that MPTCP is by default done depending on the "/proc/sys/net/mptcp/enabled" sysctl.

    NetworkManager does not change the MPTCP limits nor enable MPTCP via "/proc/sys/net/mptcp/enabled". That is a host configuration which the admin can change via sysctl and ip-mptcp.

    Strict reverse path filtering (rp_filter) breaks many MPTCP use cases, so when MPTCP handling for IPv4 addresses on the interface is enabled, NetworkManager would loosen the strict reverse path filtering (1) to the loose setting (2).

    Format: uint32

connection.mud-url
    If configured, set to a Manufacturer Usage Description (MUD) URL that points to manufacturer-recommended network policies for IoT devices. It is transmitted as a DHCPv4 or DHCPv6 option. The value must be a valid URL starting with "https://".

    The special value "none" is allowed to indicate that no MUD URL is used.

    If the per-profile value is unspecified (the default), a global connection default gets consulted. If still unspecified, the ultimate default is "none".

    Format: string

connection.multi-connect
    Specifies whether the profile can be active multiple times at a particular moment. The value is of type NMConnectionMultiConnect.

    Format: int32

connection.permissions
    An array of strings defining what access a given user has to this connection. If this is NULL or empty, all users are allowed to access this connection; otherwise users are allowed if and only if they are in this list. When this is not empty, the connection can be active only when one of the specified users is logged into an active session. Each entry is of the form "[type]:[id]:[reserved]"; for example, "user:dcbw:blah".

    At this time only the "user" [type] is allowed. Any other values are ignored and reserved for future use. [id] is the username that this permission refers to, which may not contain the ":" character. Any [reserved] information present must be ignored and is reserved for future use. All of [type], [id], and [reserved] must be valid UTF-8.

    Format: array of string

connection.secondaries
    List of connection UUIDs that should be activated when the base connection itself is activated. Currently, only VPN connections are supported.

    Format: array of string

connection.slave-type
    Alias: slave-type

    Setting name of the device type of this slave's master connection (eg, "bond"), or NULL if this connection is not a slave.

    Format: string

connection.stable-id
    This represents the identity of the connection used for various purposes. It allows to configure multiple profiles to share the identity. Also, the stable-id can contain placeholders that are substituted dynamically and deterministically depending on the context.

    The stable-id is used for generating IPv6 stable private addresses with ipv6.addr-gen-mode=stable-privacy. It is also used to seed the generated cloned MAC address for ethernet.cloned-mac-address=stable and wifi.cloned-mac-address=stable. It is also used to derive the DHCP client identifier with ipv4.dhcp-client-id=stable, the DHCPv6 DUID with ipv6.dhcp-duid=stable-[llt,ll,uuid] and the DHCP IAID with ipv4.iaid=stable and ipv6.iaid=stable.

    Note that depending on the context where it is used, other parameters are also seeded into the generation algorithm. For example, a per-host key is commonly also included, so that different systems end up generating different IDs. Or with ipv6.addr-gen-mode=stable-privacy, also the device's name is included, so that different interfaces yield different addresses. The per-host key is the identity of your machine and stored in /var/lib/NetworkManager/secret_key. See NetworkManager(8) manual about the secret-key and the host identity.

    The '$' character is treated special to perform dynamic substitutions at activation time. Currently, supported are "${CONNECTION}", "${DEVICE}", "${MAC}", "${BOOT}", "${RANDOM}". These effectively create unique IDs per-connection, per-device, per-boot, or every time. The "${CONNECTION}" uses the profile's connection.uuid, the "${DEVICE}" uses the interface name of the device and "${MAC}" the permanent MAC address of the device. Any unrecognized patterns following '$' are treated verbatim, however are reserved for future use. You are thus advised to avoid '$' or escape it as "$$". For example, set it to "${CONNECTION}-${BOOT}-${DEVICE}" to create a unique id for this connection that changes with every reboot and differs depending on the interface where the profile activates.

    If the value is unset, a global connection default is consulted. If the value is still unset, the default is "default${CONNECTION}" go generate an ID unique per connection profile.

    Format: string

connection.timestamp
    The time, in seconds since the Unix Epoch, that the connection was last _successfully_ fully activated.

    NetworkManager updates the connection timestamp periodically when the connection is active to ensure that an active connection has the latest timestamp. The property is only meant for reading (changes to this property will not be preserved).

    Format: uint64

connection.type
    Alias: type

    Base type of the connection. For hardware-dependent connections, should contain the setting name of the hardware-type specific setting (ie, "802-3-ethernet" or "802-11-wireless" or "bluetooth", etc), and for non-hardware dependent connections like VPN or otherwise, should contain the setting name of that setting type (ie, "vpn" or "bridge", etc).

    Format: string

connection.uuid
    A universally unique identifier for the connection, for example generated with libuuid. It should be assigned when the connection is created, and never changed as long as the connection still applies to the same network. For example, it should not be changed when the "id" property or NMSettingIP4Config changes, but might need to be re-created when the Wi-Fi SSID, mobile broadband network provider, or "type" property changes.

    The UUID must be in the format "2815492f-7e56-435e-b2e9-246bd7cdc664" (ie, contains only hexadecimal characters and "-").

    Format: a valid RFC4122 universally unique identifier (UUID).

connection.wait-activation-delay
    Time in milliseconds to wait for connection to be considered activated. The wait will start after the pre-up dispatcher event.

    The value 0 means no wait time. The default value is -1, which currently has the same meaning as no wait time.

    Format: int32

connection.wait-device-timeout
    Timeout in milliseconds to wait for device at startup. During boot, devices may take a while to be detected by the driver. This property will cause to delay NetworkManager-wait-online.service and nm-online to give the device a chance to appear. This works by waiting for the given timeout until a compatible device for the profile is available and managed.

    The value 0 means no wait time. The default value is -1, which currently has the same meaning as no wait time.

    Format: int32

connection.zone
    The trust level of a the connection. Free form case-insensitive string (for example "Home", "Work", "Public"). NULL or unspecified zone means the connection will be placed in the default zone as defined by the firewall.

    When updating this property on a currently activated connection, the change takes effect immediately.

    Format: string

  6lowpan setting

6LoWPAN Settings.

Properties:

6lowpan.parent
    Alias: dev

    If given, specifies the parent interface name or parent connection UUID from which this 6LowPAN interface should be created.

    Format: string

  802-1x setting

IEEE 802.1x Authentication Settings.

Properties:

802-1x.altsubject-matches
    List of strings to be matched against the altSubjectName of the certificate presented by the authentication server. If the list is empty, no verification of the server certificate's altSubjectName is performed.

    Format: array of string

802-1x.anonymous-identity
    Anonymous identity string for EAP authentication methods. Used as the unencrypted identity with EAP types that support different tunneled identity like EAP-TTLS.

    Format: string

802-1x.auth-timeout
    A timeout for the authentication. Zero means the global default; if the global default is not set, the authentication timeout is 25 seconds.

    Format: int32

802-1x.ca-cert
    Contains the CA certificate if used by the EAP method specified in the "eap" property.

    Certificate data is specified using a "scheme"; three are currently supported: blob, path and pkcs#11 URL. When using the blob scheme this property should be set to the certificate's DER encoded data. When using the path scheme, this property should be set to the full UTF-8 encoded path of the certificate, prefixed with the string "file://" and ending with a terminating NUL byte. This property can be unset even if the EAP method supports CA certificates, but this allows man-in-the-middle attacks and is NOT recommended.

    Note that enabling NMSetting8021x:system-ca-certs will override this setting to use the built-in path, if the built-in path is not a directory.

    Format: byte array

802-1x.ca-cert-password
    The password used to access the CA certificate stored in "ca-cert" property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

    Format: string

802-1x.ca-cert-password-flags
    Flags indicating how to handle the "ca-cert-password" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.ca-path
    UTF-8 encoded path to a directory containing PEM or DER formatted certificates to be added to the verification chain in addition to the certificate specified in the "ca-cert" property.

    If NMSetting8021x:system-ca-certs is enabled and the built-in CA path is an existing directory, then this setting is ignored.

    Format: string

802-1x.client-cert
    Contains the client certificate if used by the EAP method specified in the "eap" property.

    Certificate data is specified using a "scheme"; two are currently supported: blob and path. When using the blob scheme (which is backwards compatible with NM 0.7.x) this property should be set to the certificate's DER encoded data. When using the path scheme, this property should be set to the full UTF-8 encoded path of the certificate, prefixed with the string "file://" and ending with a terminating NUL byte.

    Format: byte array

802-1x.client-cert-password
    The password used to access the client certificate stored in "client-cert" property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

    Format: string

802-1x.client-cert-password-flags
    Flags indicating how to handle the "client-cert-password" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.domain-match
    Constraint for server domain name. If set, this list of FQDNs is used as a match requirement for dNSName element(s) of the certificate presented by the authentication server. If a matching dNSName is found, this constraint is met. If no dNSName values are present, this constraint is matched against SubjectName CN using the same comparison. Multiple valid FQDNs can be passed as a ";" delimited list.

    Format: string

802-1x.domain-suffix-match
    Constraint for server domain name. If set, this FQDN is used as a suffix match requirement for dNSName element(s) of the certificate presented by the authentication server. If a matching dNSName is found, this constraint is met. If no dNSName values are present, this constraint is matched against SubjectName CN using same suffix match comparison. Since version 1.24, multiple valid FQDNs can be passed as a ";" delimited list.

    Format: string

802-1x.eap
    The allowed EAP method to be used when authenticating to the network with 802.1x. Valid methods are: "leap", "md5", "tls", "peap", "ttls", "pwd", and "fast". Each method requires different configuration using the properties of this setting; refer to wpa_supplicant documentation for the allowed combinations.

    Format: array of string

802-1x.identity
    Identity string for EAP authentication methods. Often the user's user or login name.

    Format: string

802-1x.optional
    Whether the 802.1X authentication is optional. If TRUE, the activation will continue even after a timeout or an authentication failure. Setting the property to TRUE is currently allowed only for Ethernet connections. If set to FALSE, the activation can continue only after a successful authentication.

    Format: boolean

802-1x.pac-file
    UTF-8 encoded file path containing PAC for EAP-FAST.

    Format: string

802-1x.password
    UTF-8 encoded password used for EAP authentication methods. If both the "password" property and the "password-raw" property are specified, "password" is preferred.

    Format: string

802-1x.password-flags
    Flags indicating how to handle the "password" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.password-raw
    Password used for EAP authentication methods, given as a byte array to allow passwords in other encodings than UTF-8 to be used. If both the "password" property and the "password-raw" property are specified, "password" is preferred.

    Format: byte array

802-1x.password-raw-flags
    Flags indicating how to handle the "password-raw" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.phase1-auth-flags
    Specifies authentication flags to use in "phase 1" outer authentication using NMSetting8021xAuthFlags options. The individual TLS versions can be explicitly disabled. TLS time checks can be also disabled. If a certain TLS disable flag is not set, it is up to the supplicant to allow or forbid it. The TLS options map to tls_disable_tlsv1_x and tls_disable_time_checks settings. See the wpa_supplicant documentation for more details.

    Format: uint32

802-1x.phase1-fast-provisioning
    Enables or disables in-line provisioning of EAP-FAST credentials when FAST is specified as the EAP method in the "eap" property. Recognized values are "0" (disabled), "1" (allow unauthenticated provisioning), "2" (allow authenticated provisioning), and "3" (allow both authenticated and unauthenticated provisioning). See the wpa_supplicant documentation for more details.

    Format: string

802-1x.phase1-peaplabel
    Forces use of the new PEAP label during key derivation. Some RADIUS servers may require forcing the new PEAP label to interoperate with PEAPv1. Set to "1" to force use of the new PEAP label. See the wpa_supplicant documentation for more details.

    Format: string

802-1x.phase1-peapver
    Forces which PEAP version is used when PEAP is set as the EAP method in the "eap" property. When unset, the version reported by the server will be used. Sometimes when using older RADIUS servers, it is necessary to force the client to use a particular PEAP version. To do so, this property may be set to "0" or "1" to force that specific PEAP version.

    Format: string

802-1x.phase2-altsubject-matches
    List of strings to be matched against the altSubjectName of the certificate presented by the authentication server during the inner "phase 2" authentication. If the list is empty, no verification of the server certificate's altSubjectName is performed.

    Format: array of string

802-1x.phase2-auth
    Specifies the allowed "phase 2" inner authentication method when an EAP method that uses an inner TLS tunnel is specified in the "eap" property. For TTLS this property selects one of the supported non-EAP inner methods: "pap", "chap", "mschap", "mschapv2" while "phase2-autheap" selects an EAP inner method. For PEAP this selects an inner EAP method, one of: "gtc", "otp", "md5" and "tls". Each "phase 2" inner method requires specific parameters for successful authentication; see the wpa_supplicant documentation for more details. Both "phase2-auth" and "phase2-autheap" cannot be specified.

    Format: string

802-1x.phase2-autheap
    Specifies the allowed "phase 2" inner EAP-based authentication method when TTLS is specified in the "eap" property. Recognized EAP-based "phase 2" methods are "md5", "mschapv2", "otp", "gtc", and "tls". Each "phase 2" inner method requires specific parameters for successful authentication; see the wpa_supplicant documentation for more details.

    Format: string

802-1x.phase2-ca-cert
    Contains the "phase 2" CA certificate if used by the EAP method specified in the "phase2-auth" or "phase2-autheap" properties.

    Certificate data is specified using a "scheme"; three are currently supported: blob, path and pkcs#11 URL. When using the blob scheme this property should be set to the certificate's DER encoded data. When using the path scheme, this property should be set to the full UTF-8 encoded path of the certificate, prefixed with the string "file://" and ending with a terminating NUL byte. This property can be unset even if the EAP method supports CA certificates, but this allows man-in-the-middle attacks and is NOT recommended.

    Note that enabling NMSetting8021x:system-ca-certs will override this setting to use the built-in path, if the built-in path is not a directory.

    Format: byte array

802-1x.phase2-ca-cert-password
    The password used to access the "phase2" CA certificate stored in "phase2-ca-cert" property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

    Format: string

802-1x.phase2-ca-cert-password-flags
    Flags indicating how to handle the "phase2-ca-cert-password" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.phase2-ca-path
    UTF-8 encoded path to a directory containing PEM or DER formatted certificates to be added to the verification chain in addition to the certificate specified in the "phase2-ca-cert" property.

    If NMSetting8021x:system-ca-certs is enabled and the built-in CA path is an existing directory, then this setting is ignored.

    Format: string

802-1x.phase2-client-cert
    Contains the "phase 2" client certificate if used by the EAP method specified in the "phase2-auth" or "phase2-autheap" properties.

    Certificate data is specified using a "scheme"; two are currently supported: blob and path. When using the blob scheme (which is backwards compatible with NM 0.7.x) this property should be set to the certificate's DER encoded data. When using the path scheme, this property should be set to the full UTF-8 encoded path of the certificate, prefixed with the string "file://" and ending with a terminating NUL byte. This property can be unset even if the EAP method supports CA certificates, but this allows man-in-the-middle attacks and is NOT recommended.

    Format: byte array

802-1x.phase2-client-cert-password
    The password used to access the "phase2" client certificate stored in "phase2-client-cert" property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

    Format: string

802-1x.phase2-client-cert-password-flags
    Flags indicating how to handle the "phase2-client-cert-password" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.phase2-domain-match
    Constraint for server domain name. If set, this list of FQDNs is used as a match requirement for dNSName element(s) of the certificate presented by the authentication server during the inner "phase 2" authentication. If a matching dNSName is found, this constraint is met. If no dNSName values are present, this constraint is matched against SubjectName CN using the same comparison. Multiple valid FQDNs can be passed as a ";" delimited list.

    Format: string

802-1x.phase2-domain-suffix-match
    Constraint for server domain name. If set, this FQDN is used as a suffix match requirement for dNSName element(s) of the certificate presented by the authentication server during the inner "phase 2" authentication. If a matching dNSName is found, this constraint is met. If no dNSName values are present, this constraint is matched against SubjectName CN using same suffix match comparison. Since version 1.24, multiple valid FQDNs can be passed as a ";" delimited list.

    Format: string

802-1x.phase2-private-key
    Contains the "phase 2" inner private key when the "phase2-auth" or "phase2-autheap" property is set to "tls".

    Key data is specified using a "scheme"; two are currently supported: blob and path. When using the blob scheme and private keys, this property should be set to the key's encrypted PEM encoded data. When using private keys with the path scheme, this property should be set to the full UTF-8 encoded path of the key, prefixed with the string "file://" and ending with a terminating NUL byte. When using PKCS#12 format private keys and the blob scheme, this property should be set to the PKCS#12 data and the "phase2-private-key-password" property must be set to password used to decrypt the PKCS#12 certificate and key. When using PKCS#12 files and the path scheme, this property should be set to the full UTF-8 encoded path of the key, prefixed with the string "file://" and ending with a terminating NUL byte, and as with the blob scheme the "phase2-private-key-password" property must be set to the password used to decode the PKCS#12 private key and certificate.

    Format: byte array

802-1x.phase2-private-key-password
    The password used to decrypt the "phase 2" private key specified in the "phase2-private-key" property when the private key either uses the path scheme, or is a PKCS#12 format key.

    Format: string

802-1x.phase2-private-key-password-flags
    Flags indicating how to handle the "phase2-private-key-password" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.phase2-subject-match
    Substring to be matched against the subject of the certificate presented by the authentication server during the inner "phase 2" authentication. When unset, no verification of the authentication server certificate's subject is performed. This property provides little security, if any, and should not be used.

    This property is deprecated since version 1.2. Use "phase2-domain-suffix-match" instead.

    Format: string

802-1x.pin
    PIN used for EAP authentication methods.

    Format: string

802-1x.pin-flags
    Flags indicating how to handle the "pin" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.private-key
    Contains the private key when the "eap" property is set to "tls".

    Key data is specified using a "scheme"; two are currently supported: blob and path. When using the blob scheme and private keys, this property should be set to the key's encrypted PEM encoded data. When using private keys with the path scheme, this property should be set to the full UTF-8 encoded path of the key, prefixed with the string "file://" and ending with a terminating NUL byte. When using PKCS#12 format private keys and the blob scheme, this property should be set to the PKCS#12 data and the "private-key-password" property must be set to password used to decrypt the PKCS#12 certificate and key. When using PKCS#12 files and the path scheme, this property should be set to the full UTF-8 encoded path of the key, prefixed with the string "file://" and ending with a terminating NUL byte, and as with the blob scheme the "private-key-password" property must be set to the password used to decode the PKCS#12 private key and certificate.

    WARNING: "private-key" is not a "secret" property, and thus unencrypted private key data using the BLOB scheme may be readable by unprivileged users. Private keys should always be encrypted with a private key password to prevent unauthorized access to unencrypted private key data.

    Format: byte array

802-1x.private-key-password
    The password used to decrypt the private key specified in the "private-key" property when the private key either uses the path scheme, or if the private key is a PKCS#12 format key.

    Format: string

802-1x.private-key-password-flags
    Flags indicating how to handle the "private-key-password" property.

    Format: NMSettingSecretFlags (uint32)

802-1x.subject-match
    Substring to be matched against the subject of the certificate presented by the authentication server. When unset, no verification of the authentication server certificate's subject is performed. This property provides little security, if any, and should not be used.

    This property is deprecated since version 1.2. Use "phase2-domain-suffix-match" instead.

    Format: string

802-1x.system-ca-certs
    When TRUE, overrides the "ca-path" and "phase2-ca-path" properties using the system CA directory specified at configure time with the --system-ca-path switch. The certificates in this directory are added to the verification chain in addition to any certificates specified by the "ca-cert" and "phase2-ca-cert" properties. If the path provided with --system-ca-path is rather a file name (bundle of trusted CA certificates), it overrides "ca-cert" and "phase2-ca-cert" properties instead (sets ca_cert/ca_cert2 options for wpa_supplicant).

    Format: boolean

  adsl setting

ADSL Settings.

Properties:

adsl.encapsulation
    Alias: encapsulation

    Encapsulation of ADSL connection. Can be "vcmux" or "llc".

    Format: string

adsl.password
    Alias: password

    Password used to authenticate with the ADSL service.

    Format: string

adsl.password-flags
    Flags indicating how to handle the "password" property.

    Format: NMSettingSecretFlags (uint32)

adsl.protocol
    Alias: protocol

    ADSL connection protocol. Can be "pppoa", "pppoe" or "ipoatm".

    Format: string

adsl.username
    Alias: username

    Username used to authenticate with the ADSL service.

    Format: string

adsl.vci
    VCI of ADSL connection

    Format: uint32

adsl.vpi
    VPI of ADSL connection

    Format: uint32

  bluetooth setting

Bluetooth Settings.

Properties:

bluetooth.bdaddr
    Alias: addr

    The Bluetooth address of the device.

    Format: byte array

bluetooth.type
    Alias: bt-type

    Either "dun" for Dial-Up Networking connections or "panu" for Personal Area Networking connections to devices supporting the NAP profile.

    Format: string

  bond setting

Bonding Settings.

Properties:

bond.options
    Dictionary of key/value pairs of bonding options. Both keys and values must be strings. Option names must contain only alphanumeric characters (ie, [a-zA-Z0-9]).

    Format: dict of string to string

  bridge setting

Bridging Settings.

Properties:

bridge.ageing-time
    Alias: ageing-time

    The Ethernet MAC address aging time, in seconds.

    Format: uint32

bridge.forward-delay
    Alias: forward-delay

    The Spanning Tree Protocol (STP) forwarding delay, in seconds.

    Format: uint32

bridge.group-address
    If specified, The MAC address of the multicast group this bridge uses for STP.

    The address must be a link-local address in standard Ethernet MAC address format, ie an address of the form 01:80:C2:00:00:0X, with X in [0, 4..F]. If not specified the default value is 01:80:C2:00:00:00.

    Format: byte array

bridge.group-forward-mask
    Alias: group-forward-mask

    A mask of group addresses to forward. Usually, group addresses in the range from 01:80:C2:00:00:00 to 01:80:C2:00:00:0F are not forwarded according to standards. This property is a mask of 16 bits, each corresponding to a group address in that range that must be forwarded. The mask can't have bits 0, 1 or 2 set because they are used for STP, MAC pause frames and LACP.

    Format: uint32

bridge.hello-time
    Alias: hello-time

    The Spanning Tree Protocol (STP) hello time, in seconds.

    Format: uint32

bridge.mac-address
    Alias: mac

    If specified, the MAC address of bridge. When creating a new bridge, this MAC address will be set.

    If this field is left unspecified, the "ethernet.cloned-mac-address" is referred instead to generate the initial MAC address. Note that setting "ethernet.cloned-mac-address" anyway overwrites the MAC address of the bridge later while activating the bridge.

    This property is deprecated since version 1.12. Use the "cloned-mac-address" property instead.

    Format: byte array

bridge.max-age
    Alias: max-age

    The Spanning Tree Protocol (STP) maximum message age, in seconds.

    Format: uint32

bridge.multicast-hash-max
    Set maximum size of multicast hash table (value must be a power of 2).

    Format: uint32

bridge.multicast-last-member-count
    Set the number of queries the bridge will send before stopping forwarding a multicast group after a "leave" message has been received.

    Format: uint32

bridge.multicast-last-member-interval
    Set interval (in deciseconds) between queries to find remaining members of a group, after a "leave" message is received.

    Format: uint64

bridge.multicast-membership-interval
    Set delay (in deciseconds) after which the bridge will leave a group, if no membership reports for this group are received.

    Format: uint64

bridge.multicast-querier
    Enable or disable sending of multicast queries by the bridge. If not specified the option is disabled.

    Format: boolean

bridge.multicast-querier-interval
    If no queries are seen after this delay (in deciseconds) has passed, the bridge will start to send its own queries.

    Format: uint64

bridge.multicast-query-interval
    Interval (in deciseconds) between queries sent by the bridge after the end of the startup phase.

    Format: uint64

bridge.multicast-query-response-interval
    Set the Max Response Time/Max Response Delay (in deciseconds) for IGMP/MLD queries sent by the bridge.

    Format: uint64

bridge.multicast-query-use-ifaddr
    If enabled the bridge's own IP address is used as the source address for IGMP queries otherwise the default of 0.0.0.0 is used.

    Format: boolean

bridge.multicast-router
    Sets bridge's multicast router. Multicast-snooping must be enabled for this option to work.

    Supported values are: 'auto', 'disabled', 'enabled' to which kernel assigns the numbers 1, 0, and 2, respectively. If not specified the default value is 'auto' (1).

    Format: string

bridge.multicast-snooping
    Alias: multicast-snooping

    Controls whether IGMP snooping is enabled for this bridge. Note that if snooping was automatically disabled due to hash collisions, the system may refuse to enable the feature until the collisions are resolved.

    Format: boolean

bridge.multicast-startup-query-count
    Set the number of IGMP queries to send during startup phase.

    Format: uint32

bridge.multicast-startup-query-interval
    Sets the time (in deciseconds) between queries sent out at startup to determine membership information.

    Format: uint64

bridge.priority
    Alias: priority

    Sets the Spanning Tree Protocol (STP) priority for this bridge. Lower values are "better"; the lowest priority bridge will be elected the root bridge.

    Format: uint32

bridge.stp
    Alias: stp

    Controls whether Spanning Tree Protocol (STP) is enabled for this bridge.

    Format: boolean

bridge.vlan-default-pvid
    The default PVID for the ports of the bridge, that is the VLAN id assigned to incoming untagged frames.

    Format: uint32

bridge.vlan-filtering
    Control whether VLAN filtering is enabled on the bridge.

    Format: boolean

bridge.vlan-protocol
    If specified, the protocol used for VLAN filtering.

    Supported values are: '802.1Q', '802.1ad'. If not specified the default value is '802.1Q'.

    Format: string

bridge.vlan-stats-enabled
    Controls whether per-VLAN stats accounting is enabled.

    Format: boolean

bridge.vlans
    Array of bridge VLAN objects. In addition to the VLANs specified here, the bridge will also have the default-pvid VLAN configured by the bridge.vlan-default-pvid property.

    In nmcli the VLAN list can be specified with the following syntax:

    $vid [pvid] [untagged] [, $vid [pvid] [untagged]]...

    where $vid is either a single id between 1 and 4094 or a range, represented as a couple of ids separated by a dash.

    Format: array of vardict

  bridge-port setting

Bridge Port Settings.

Properties:

bridge-port.hairpin-mode
    Alias: hairpin

    Enables or disables "hairpin mode" for the port, which allows frames to be sent back out through the port the frame was received on.

    Format: boolean

bridge-port.path-cost
    Alias: path-cost

    The Spanning Tree Protocol (STP) port cost for destinations via this port.

    Format: uint32

bridge-port.priority
    Alias: priority

    The Spanning Tree Protocol (STP) priority of this bridge port.

    Format: uint32

bridge-port.vlans
    Array of bridge VLAN objects. In addition to the VLANs specified here, the port will also have the default-pvid VLAN configured on the bridge by the bridge.vlan-default-pvid property.

    In nmcli the VLAN list can be specified with the following syntax:

    $vid [pvid] [untagged] [, $vid [pvid] [untagged]]...

    where $vid is either a single id between 1 and 4094 or a range, represented as a couple of ids separated by a dash.

    Format: array of vardict

  cdma setting

CDMA-based Mobile Broadband Settings.

Properties:

cdma.mtu
    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple frames.

    Format: uint32

cdma.number
    The number to dial to establish the connection to the CDMA-based mobile broadband network, if any. If not specified, the default number (#777) is used when required.

    Format: string

cdma.password
    Alias: password

    The password used to authenticate with the network, if required. Many providers do not require a password, or accept any password. But if a password is required, it is specified here.

    Format: string

cdma.password-flags
    Flags indicating how to handle the "password" property.

    Format: NMSettingSecretFlags (uint32)

cdma.username
    Alias: user

    The username used to authenticate with the network, if required. Many providers do not require a username, or accept any username. But if a username is required, it is specified here.

    Format: string

  dcb setting

Data Center Bridging Settings.

Properties:

dcb.app-fcoe-flags
    Specifies the NMSettingDcbFlags for the DCB FCoE application. Flags may be any combination of NM_SETTING_DCB_FLAG_ENABLE (0x1), NM_SETTING_DCB_FLAG_ADVERTISE (0x2), and NM_SETTING_DCB_FLAG_WILLING (0x4).

    Format: NMSettingDcbFlags (uint32)

dcb.app-fcoe-mode
    The FCoE controller mode; either "fabric" or "vn2vn".

    Since 1.34, NULL is the default and means "fabric". Before 1.34, NULL was rejected as invalid and the default was "fabric".

    Format: string

dcb.app-fcoe-priority
    The highest User Priority (0 - 7) which FCoE frames should use, or -1 for default priority. Only used when the "app-fcoe-flags" property includes the NM_SETTING_DCB_FLAG_ENABLE (0x1) flag.

    Format: int32

dcb.app-fip-flags
    Specifies the NMSettingDcbFlags for the DCB FIP application. Flags may be any combination of NM_SETTING_DCB_FLAG_ENABLE (0x1), NM_SETTING_DCB_FLAG_ADVERTISE (0x2), and NM_SETTING_DCB_FLAG_WILLING (0x4).

    Format: NMSettingDcbFlags (uint32)

dcb.app-fip-priority
    The highest User Priority (0 - 7) which FIP frames should use, or -1 for default priority. Only used when the "app-fip-flags" property includes the NM_SETTING_DCB_FLAG_ENABLE (0x1) flag.

    Format: int32

dcb.app-iscsi-flags
    Specifies the NMSettingDcbFlags for the DCB iSCSI application. Flags may be any combination of NM_SETTING_DCB_FLAG_ENABLE (0x1), NM_SETTING_DCB_FLAG_ADVERTISE (0x2), and NM_SETTING_DCB_FLAG_WILLING (0x4).

    Format: NMSettingDcbFlags (uint32)

dcb.app-iscsi-priority
    The highest User Priority (0 - 7) which iSCSI frames should use, or -1 for default priority. Only used when the "app-iscsi-flags" property includes the NM_SETTING_DCB_FLAG_ENABLE (0x1) flag.

    Format: int32

dcb.priority-bandwidth
    An array of 8 uint values, where the array index corresponds to the User Priority (0 - 7) and the value indicates the percentage of bandwidth of the priority's assigned group that the priority may use. The sum of all percentages for priorities which belong to the same group must total 100 percents.

    Format: array of uint32

dcb.priority-flow-control
    An array of 8 boolean values, where the array index corresponds to the User Priority (0 - 7) and the value indicates whether or not the corresponding priority should transmit priority pause.

    Format: array of uint32

dcb.priority-flow-control-flags
    Specifies the NMSettingDcbFlags for DCB Priority Flow Control (PFC). Flags may be any combination of NM_SETTING_DCB_FLAG_ENABLE (0x1), NM_SETTING_DCB_FLAG_ADVERTISE (0x2), and NM_SETTING_DCB_FLAG_WILLING (0x4).

    Format: NMSettingDcbFlags (uint32)

dcb.priority-group-bandwidth
    An array of 8 uint values, where the array index corresponds to the Priority Group ID (0 - 7) and the value indicates the percentage of link bandwidth allocated to that group. Allowed values are 0 - 100, and the sum of all values must total 100 percents.

    Format: array of uint32

dcb.priority-group-flags
    Specifies the NMSettingDcbFlags for DCB Priority Groups. Flags may be any combination of NM_SETTING_DCB_FLAG_ENABLE (0x1), NM_SETTING_DCB_FLAG_ADVERTISE (0x2), and NM_SETTING_DCB_FLAG_WILLING (0x4).

    Format: NMSettingDcbFlags (uint32)

dcb.priority-group-id
    An array of 8 uint values, where the array index corresponds to the User Priority (0 - 7) and the value indicates the Priority Group ID. Allowed Priority Group ID values are 0 - 7 or 15 for the unrestricted group.

    Format: array of uint32

dcb.priority-strict-bandwidth
    An array of 8 boolean values, where the array index corresponds to the User Priority (0 - 7) and the value indicates whether or not the priority may use all of the bandwidth allocated to its assigned group.

    Format: array of uint32

dcb.priority-traffic-class
    An array of 8 uint values, where the array index corresponds to the User Priority (0 - 7) and the value indicates the traffic class (0 - 7) to which the priority is mapped.

    Format: array of uint32

  ethtool setting

Ethtool Ethernet Settings.

Properties:

ethtool.coalesce-adaptive-rx

ethtool.coalesce-adaptive-tx

ethtool.coalesce-pkt-rate-high

ethtool.coalesce-pkt-rate-low

ethtool.coalesce-rx-frames

ethtool.coalesce-rx-frames-high

ethtool.coalesce-rx-frames-irq

ethtool.coalesce-rx-frames-low

ethtool.coalesce-rx-usecs

ethtool.coalesce-rx-usecs-high

ethtool.coalesce-rx-usecs-irq

ethtool.coalesce-rx-usecs-low

ethtool.coalesce-sample-interval

ethtool.coalesce-stats-block-usecs

ethtool.coalesce-tx-frames

ethtool.coalesce-tx-frames-high

ethtool.coalesce-tx-frames-irq

ethtool.coalesce-tx-frames-low

ethtool.coalesce-tx-usecs

ethtool.coalesce-tx-usecs-high

ethtool.coalesce-tx-usecs-irq

ethtool.coalesce-tx-usecs-low

ethtool.feature-esp-hw-offload

ethtool.feature-esp-tx-csum-hw-offload

ethtool.feature-fcoe-mtu

ethtool.feature-gro

ethtool.feature-gso

ethtool.feature-highdma

ethtool.feature-hw-tc-offload

ethtool.feature-l2-fwd-offload

ethtool.feature-loopback

ethtool.feature-lro

ethtool.feature-macsec-hw-offload

ethtool.feature-ntuple

ethtool.feature-rx

ethtool.feature-rx-all

ethtool.feature-rx-fcs

ethtool.feature-rx-gro-hw

ethtool.feature-rx-gro-list

ethtool.feature-rx-udp-gro-forwarding

ethtool.feature-rx-udp_tunnel-port-offload

ethtool.feature-rx-vlan-filter

ethtool.feature-rx-vlan-stag-filter

ethtool.feature-rx-vlan-stag-hw-parse

ethtool.feature-rxhash

ethtool.feature-rxvlan

ethtool.feature-sg

ethtool.feature-tls-hw-record

ethtool.feature-tls-hw-rx-offload

ethtool.feature-tls-hw-tx-offload

ethtool.feature-tso

ethtool.feature-tx

ethtool.feature-tx-checksum-fcoe-crc

ethtool.feature-tx-checksum-ip-generic

ethtool.feature-tx-checksum-ipv4

ethtool.feature-tx-checksum-ipv6

ethtool.feature-tx-checksum-sctp

ethtool.feature-tx-esp-segmentation

ethtool.feature-tx-fcoe-segmentation

ethtool.feature-tx-gre-csum-segmentation

ethtool.feature-tx-gre-segmentation

ethtool.feature-tx-gso-list

ethtool.feature-tx-gso-partial

ethtool.feature-tx-gso-robust

ethtool.feature-tx-ipxip4-segmentation

ethtool.feature-tx-ipxip6-segmentation

ethtool.feature-tx-nocache-copy

ethtool.feature-tx-scatter-gather

ethtool.feature-tx-scatter-gather-fraglist

ethtool.feature-tx-sctp-segmentation

ethtool.feature-tx-tcp-ecn-segmentation

ethtool.feature-tx-tcp-mangleid-segmentation

ethtool.feature-tx-tcp-segmentation

ethtool.feature-tx-tcp6-segmentation

ethtool.feature-tx-tunnel-remcsum-segmentation

ethtool.feature-tx-udp-segmentation

ethtool.feature-tx-udp_tnl-csum-segmentation

ethtool.feature-tx-udp_tnl-segmentation

ethtool.feature-tx-vlan-stag-hw-insert

ethtool.feature-txvlan

ethtool.pause-autoneg

ethtool.pause-rx

ethtool.pause-tx

ethtool.ring-rx

ethtool.ring-rx-jumbo

ethtool.ring-rx-mini

ethtool.ring-tx

  gsm setting

GSM-based Mobile Broadband Settings.

Properties:

gsm.apn
    Alias: apn

    The GPRS Access Point Name specifying the APN used when establishing a data session with the GSM-based network. The APN often determines how the user will be billed for their network usage and whether the user has access to the Internet or just a provider-specific walled-garden, so it is important to use the correct APN for the user's mobile broadband plan. The APN may only be composed of the characters a-z, 0-9, ., and - per GSM 03.60 Section 14.9.

    Format: string

gsm.auto-config
    When TRUE, the settings such as APN, username, or password will default to values that match the network the modem will register to in the Mobile Broadband Provider database.

    Format: boolean

gsm.device-id
    The device unique identifier (as given by the WWAN management service) which this connection applies to. If given, the connection will only apply to the specified device.

    Format: string

gsm.home-only
    When TRUE, only connections to the home network will be allowed. Connections to roaming networks will not be made.

    Format: boolean

gsm.initial-eps-bearer-apn
    For LTE modems, this sets the APN for the initial EPS bearer that is set up when attaching to the network. Setting this parameter implies initial-eps-bearer-configure to be TRUE.

    Format: string

gsm.initial-eps-bearer-configure
    For LTE modems, this setting determines whether the initial EPS bearer shall be configured when bringing up the connection. It is inferred TRUE if initial-eps-bearer-apn is set.

    Format: boolean

gsm.mtu
    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple frames.

    Format: uint32

gsm.network-id
    The Network ID (GSM LAI format, ie MCC-MNC) to force specific network registration. If the Network ID is specified, NetworkManager will attempt to force the device to register only on the specified network. This can be used to ensure that the device does not roam when direct roaming control of the device is not otherwise possible.

    Format: string

gsm.number
    Legacy setting that used to help establishing PPP data sessions for GSM-based modems.

    This property is deprecated since version 1.16. User-provided values for this setting are no longer used.

    Format: string

gsm.password
    Alias: password

    The password used to authenticate with the network, if required. Many providers do not require a password, or accept any password. But if a password is required, it is specified here.

    Format: string

gsm.password-flags
    Flags indicating how to handle the "password" property.

    Format: NMSettingSecretFlags (uint32)

gsm.pin
    If the SIM is locked with a PIN it must be unlocked before any other operations are requested. Specify the PIN here to allow operation of the device.

    Format: string

gsm.pin-flags
    Flags indicating how to handle the "pin" property.

    Format: NMSettingSecretFlags (uint32)

gsm.sim-id
    The SIM card unique identifier (as given by the WWAN management service) which this connection applies to. If given, the connection will apply to any device also allowed by "device-id" which contains a SIM card matching the given identifier.

    Format: string

gsm.sim-operator-id
    A MCC/MNC string like "310260" or "21601" identifying the specific mobile network operator which this connection applies to. If given, the connection will apply to any device also allowed by "device-id" and "sim-id" which contains a SIM card provisioned by the given operator.

    Format: string

gsm.username
    Alias: user

    The username used to authenticate with the network, if required. Many providers do not require a username, or accept any username. But if a username is required, it is specified here.

    Format: string

  infiniband setting

Infiniband Settings.

Properties:

infiniband.mac-address
    Alias: mac

    If specified, this connection will only apply to the IPoIB device whose permanent MAC address matches. This property does not change the MAC address of the device (i.e. MAC spoofing).

    Format: byte array

infiniband.mtu
    Alias: mtu

    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple frames.

    Format: uint32

infiniband.p-key
    Alias: p-key

    The InfiniBand P_Key to use for this device. A value of -1 means to use the default P_Key (aka "the P_Key at index 0"). Otherwise, it is a 16-bit unsigned integer, whose high bit is set if it is a "full membership" P_Key.

    Format: int32

infiniband.parent
    Alias: parent

    The interface name of the parent device of this device. Normally NULL, but if the "p_key" property is set, then you must specify the base device by setting either this property or "mac-address".

    Format: string

infiniband.transport-mode
    Alias: transport-mode

    The IP-over-InfiniBand transport mode. Either "datagram" or "connected".

    Format: string

  ipv4 setting

IPv4 Settings.

Properties:

ipv4.addresses
    Alias: ip4

    Array of IP addresses.

    Format: a comma separated list of addresses

ipv4.auto-route-ext-gw
    VPN connections will default to add the route automatically unless this setting is set to FALSE.

    For other connection types, adding such an automatic route is currently not supported and setting this to TRUE has no effect.

    Format: NMTernary (int32)

ipv4.dad-timeout
    Timeout in milliseconds used to check for the presence of duplicate IP addresses on the network. If an address conflict is detected, the activation will fail. A zero value means that no duplicate address detection is performed, -1 means the default value (either configuration ipvx.dad-timeout override or zero). A value greater than zero is a timeout in milliseconds.

    The property is currently implemented only for IPv4.

    Format: int32

ipv4.dhcp-client-id
    A string sent to the DHCP server to identify the local machine which the DHCP server may use to customize the DHCP lease and options. When the property is a hex string ('aa:bb:cc') it is interpreted as a binary client ID, in which case the first byte is assumed to be the 'type' field as per RFC 2132 section 9.14 and the remaining bytes may be an hardware address (e.g. '01:xx:xx:xx:xx:xx:xx' where 1 is the Ethernet ARP type and the rest is a MAC address). If the property is not a hex string it is considered as a non-hardware-address client ID and the 'type' field is set to 0.

    The special values "mac" and "perm-mac" are supported, which use the current or permanent MAC address of the device to generate a client identifier with type ethernet (01). Currently, these options only work for ethernet type of links.

    The special value "ipv6-duid" uses the DUID from "ipv6.dhcp-duid" property as an RFC4361-compliant client identifier. As IAID it uses "ipv4.dhcp-iaid" and falls back to "ipv6.dhcp-iaid" if unset.

    The special value "duid" generates a RFC4361-compliant client identifier based on "ipv4.dhcp-iaid" and uses a DUID generated by hashing /etc/machine-id.

    The special value "stable" is supported to generate a type 0 client identifier based on the stable-id (see connection.stable-id) and a per-host key. If you set the stable-id, you may want to include the "${DEVICE}" or "${MAC}" specifier to get a per-device key.

    If unset, a globally configured default is used. If still unset, the default depends on the DHCP plugin.

    Format: string

ipv4.dhcp-fqdn
    If the "dhcp-send-hostname" property is TRUE, then the specified FQDN will be sent to the DHCP server when acquiring a lease. This property and "dhcp-hostname" are mutually exclusive and cannot be set at the same time.

    Format: string

ipv4.dhcp-hostname
    If the "dhcp-send-hostname" property is TRUE, then the specified name will be sent to the DHCP server when acquiring a lease. This property and "dhcp-fqdn" are mutually exclusive and cannot be set at the same time.

    Format: string

ipv4.dhcp-hostname-flags
    Flags for the DHCP hostname and FQDN.

    Currently, this property only includes flags to control the FQDN flags set in the DHCP FQDN option. Supported FQDN flags are NM_DHCP_HOSTNAME_FLAG_FQDN_SERV_UPDATE (0x1), NM_DHCP_HOSTNAME_FLAG_FQDN_ENCODED (0x2) and NM_DHCP_HOSTNAME_FLAG_FQDN_NO_UPDATE (0x4). When no FQDN flag is set and NM_DHCP_HOSTNAME_FLAG_FQDN_CLEAR_FLAGS (0x8) is set, the DHCP FQDN option will contain no flag. Otherwise, if no FQDN flag is set and NM_DHCP_HOSTNAME_FLAG_FQDN_CLEAR_FLAGS (0x8) is not set, the standard FQDN flags are set in the request: NM_DHCP_HOSTNAME_FLAG_FQDN_SERV_UPDATE (0x1), NM_DHCP_HOSTNAME_FLAG_FQDN_ENCODED (0x2) for IPv4 and NM_DHCP_HOSTNAME_FLAG_FQDN_SERV_UPDATE (0x1) for IPv6.

    When this property is set to the default value NM_DHCP_HOSTNAME_FLAG_NONE (0x0), a global default is looked up in NetworkManager configuration. If that value is unset or also NM_DHCP_HOSTNAME_FLAG_NONE (0x0), then the standard FQDN flags described above are sent in the DHCP requests.

    Format: uint32

ipv4.dhcp-iaid
    A string containing the "Identity Association Identifier" (IAID) used by the DHCP client. The string can be a 32-bit number (either decimal, hexadecimal or as colon separated hexadecimal numbers). Alternatively it can be set to the special values "mac", "perm-mac", "ifname" or "stable". When set to "mac" (or "perm-mac"), the last 4 bytes of the current (or permanent) MAC address are used as IAID. When set to "ifname", the IAID is computed by hashing the interface name. The special value "stable" can be used to generate an IAID based on the stable-id (see connection.stable-id), a per-host key and the interface name. When the property is unset, the value from global configuration is used; if no global default is set then the IAID is assumed to be "ifname".

    For DHCPv4, the IAID is only used with "ipv4.dhcp-client-id" values "duid" and "ipv6-duid" to generate the client-id.

    For DHCPv6, note that at the moment this property is only supported by the "internal" DHCPv6 plugin. The "dhclient" DHCPv6 plugin always derives the IAID from the MAC address.

    The actually used DHCPv6 IAID for a currently activated interface is exposed in the lease information of the device.

    Format: string

ipv4.dhcp-reject-servers
    Array of servers from which DHCP offers must be rejected. This property is useful to avoid getting a lease from misconfigured or rogue servers.

    For DHCPv4, each element must be an IPv4 address, optionally followed by a slash and a prefix length (e.g. "192.168.122.0/24").

    This property is currently not implemented for DHCPv6.

    Format: array of string

ipv4.dhcp-send-hostname
    If TRUE, a hostname is sent to the DHCP server when acquiring a lease. Some DHCP servers use this hostname to update DNS databases, essentially providing a static hostname for the computer. If the "dhcp-hostname" property is NULL and this property is TRUE, the current persistent hostname of the computer is sent.

    Format: boolean

ipv4.dhcp-timeout
    A timeout for a DHCP transaction in seconds. If zero (the default), a globally configured default is used. If still unspecified, a device specific timeout is used (usually 45 seconds).

    Set to 2147483647 (MAXINT32) for infinity.

    Format: int32

ipv4.dhcp-vendor-class-identifier
    The Vendor Class Identifier DHCP option (60). Special characters in the data string may be escaped using C-style escapes, nevertheless this property cannot contain nul bytes. If the per-profile value is unspecified (the default), a global connection default gets consulted. If still unspecified, the DHCP option is not sent to the server.

    Format: string

ipv4.dns
    Array of IP addresses of DNS servers.

    For DoT (DNS over TLS), the SNI server name can be specified by appending "#example.com" to the IP address of the DNS server. This currently only has effect when using systemd-resolved.

    Format: array of uint32

ipv4.dns-options
    Array of DNS options as described in man 5 resolv.conf.

    NULL means that the options are unset and left at the default. In this case NetworkManager will use default options. This is distinct from an empty list of properties.

    The currently supported options are "attempts", "debug", "edns0", "inet6", "ip6-bytestring", "ip6-dotint", "ndots", "no-aaaa", "no-check-names", "no-ip6-dotint", "no-reload", "no-tld-query", "rotate", "single-request", "single-request-reopen", "timeout", "trust-ad", "use-vc".

    The "trust-ad" setting is only honored if the profile contributes name servers to resolv.conf, and if all contributing profiles have "trust-ad" enabled.

    When using a caching DNS plugin (dnsmasq or systemd-resolved in NetworkManager.conf) then "edns0" and "trust-ad" are automatically added.

    Format: array of string

ipv4.dns-priority
    DNS servers priority.

    The relative priority for DNS servers specified by this setting. A lower numerical value is better (higher priority).

    Negative values have the special effect of excluding other configurations with a greater numerical priority value; so in presence of at least one negative priority, only DNS servers from connections with the lowest priority value will be used. To avoid all DNS leaks, set the priority of the profile that should be used to the most negative value of all active connections profiles.

    Zero selects a globally configured default value. If the latter is missing or zero too, it defaults to 50 for VPNs (including WireGuard) and 100 for other connections.

    Note that the priority is to order DNS settings for multiple active connections. It does not disambiguate multiple DNS servers within the same connection profile.

    When multiple devices have configurations with the same priority, VPNs will be considered first, then devices with the best (lowest metric) default route and then all other devices.

    When using dns=default, servers with higher priority will be on top of resolv.conf. To prioritize a given server over another one within the same connection, just specify them in the desired order. Note that commonly the resolver tries name servers in /etc/resolv.conf in the order listed, proceeding with the next server in the list on failure. See for example the "rotate" option of the dns-options setting. If there are any negative DNS priorities, then only name servers from the devices with that lowest priority will be considered.

    When using a DNS resolver that supports Conditional Forwarding or Split DNS (with dns=dnsmasq or dns=systemd-resolved settings), each connection is used to query domains in its search list. The search domains determine which name servers to ask, and the DNS priority is used to prioritize name servers based on the domain. Queries for domains not present in any search list are routed through connections having the '~.' special wildcard domain, which is added automatically to connections with the default route (or can be added manually). When multiple connections specify the same domain, the one with the best priority (lowest numerical value) wins. If a sub domain is configured on another interface it will be accepted regardless the priority, unless parent domain on the other interface has a negative priority, which causes the sub domain to be shadowed. With Split DNS one can avoid undesired DNS leaks by properly configuring DNS priorities and the search domains, so that only name servers of the desired interface are configured.

    Format: int32

ipv4.dns-search
    List of DNS search domains. Domains starting with a tilde ('~') are considered 'routing' domains and are used only to decide the interface over which a query must be forwarded; they are not used to complete unqualified host names.

    When using a DNS plugin that supports Conditional Forwarding or Split DNS, then the search domains specify which name servers to query. This makes the behavior different from running with plain /etc/resolv.conf. For more information see also the dns-priority setting.

    When set on a profile that also enabled DHCP, the DNS search list received automatically (option 119 for DHCPv4 and option 24 for DHCPv6) gets merged with the manual list. This can be prevented by setting "ignore-auto-dns". Note that if no DNS searches are configured, the fallback will be derived from the domain from DHCP (option 15).

    Format: array of string

ipv4.gateway
    Alias: gw4

    The gateway associated with this configuration. This is only meaningful if "addresses" is also set.

    Setting the gateway causes NetworkManager to configure a standard default route with the gateway as next hop. This is ignored if "never-default" is set. An alternative is to configure the default route explicitly with a manual route and /0 as prefix length.

    Note that the gateway usually conflicts with routing that NetworkManager configures for WireGuard interfaces, so usually it should not be set in that case. See "ip4-auto-default-route".

    Format: string

ipv4.ignore-auto-dns
    When "method" is set to "auto" and this property to TRUE, automatically configured name servers and search domains are ignored and only name servers and search domains specified in the "dns" and "dns-search" properties, if any, are used.

    Format: boolean

ipv4.ignore-auto-routes
    When "method" is set to "auto" and this property to TRUE, automatically configured routes are ignored and only routes specified in the "routes" property, if any, are used.

    Format: boolean

ipv4.link-local
    Enable and disable the IPv4 link-local configuration independently of the ipv4.method configuration. This allows a link-local address (169.254.x.y/16) to be obtained in addition to other addresses, such as those manually configured or obtained from a DHCP server.

    When set to "auto", the value is dependent on "ipv4.method". When set to "default", it honors the global connection default, before falling back to "auto". Note that if "ipv4.method" is "disabled", then link local addressing is always disabled too. The default is "default".

    Format: int32

ipv4.may-fail
    If TRUE, allow overall network configuration to proceed even if the configuration specified by this property times out. Note that at least one IP configuration must succeed or overall network configuration will still fail. For example, in IPv6-only networks, setting this property to TRUE on the NMSettingIP4Config allows the overall network configuration to succeed if IPv4 configuration fails but IPv6 configuration completes successfully.

    Format: boolean

ipv4.method
    Sets the IPv4 connection method. You can set one of the following values:

        • "auto" - Enables automatic IPv4 address assignment from DHCP, PPP, or similar services.

        • "manual" - Enables the configuration of static IPv4 addresses on the interface. Note that you must set at least one IP address and subnet mask in the "ipv4.addresses" property.

        • "disabled" - Disables the IPv4 protocol in this connection profile.

        • "shared" - Provides network access to other computers. If you do not specify an IP address and subnet mask in "ipv4.addresses", NetworkManager assigns 10.42.x.1/24 to the interface. Additionally, NetworkManager starts a DHCP server and DNS forwarder. Hosts that connect to this interface will then receive an IP address from the configured range, and NetworkManager configures NAT to map client addresses to the one of the current default network connection.

        • "link-local" - Enables link-local addresses according to RFC 3927. NetworkManager assigns a random link-local address from the 169.254.0.0/16 subnet to the interface.

    Format: string

ipv4.never-default
    If TRUE, this connection will never be the default connection for this IP type, meaning it will never be assigned the default route by NetworkManager.

    Format: boolean

ipv4.replace-local-rule
    Connections will default to keep the autogenerated priority 0 local rule unless this setting is set to TRUE.

    Format: NMTernary (int32)

ipv4.required-timeout
    The minimum time interval in milliseconds for which dynamic IP configuration should be tried before the connection succeeds.

    This property is useful for example if both IPv4 and IPv6 are enabled and are allowed to fail. Normally the connection succeeds as soon as one of the two address families completes; by setting a required timeout for e.g. IPv4, one can ensure that even if IP6 succeeds earlier than IPv4, NetworkManager waits some time for IPv4 before the connection becomes active.

    Note that if "may-fail" is FALSE for the same address family, this property has no effect as NetworkManager needs to wait for the full DHCP timeout.

    A zero value means that no required timeout is present, -1 means the default value (either configuration ipvx.required-timeout override or zero).

    Format: int32

ipv4.route-metric
    The default metric for routes that don't explicitly specify a metric. The default value -1 means that the metric is chosen automatically based on the device type. The metric applies to dynamic routes, manual (static) routes that don't have an explicit metric setting, address prefix routes, and the default route. Note that for IPv6, the kernel accepts zero (0) but coerces it to 1024 (user default). Hence, setting this property to zero effectively mean setting it to 1024. For IPv4, zero is a regular value for the metric.

    Format: int64

ipv4.route-table
    Enable policy routing (source routing) and set the routing table used when adding routes.

    This affects all routes, including device-routes, IPv4LL, DHCP, SLAAC, default-routes and static routes. But note that static routes can individually overwrite the setting by explicitly specifying a non-zero routing table.

    If the table setting is left at zero, it is eligible to be overwritten via global configuration. If the property is zero even after applying the global configuration value, policy routing is disabled for the address family of this connection.

    Policy routing disabled means that NetworkManager will add all routes to the main table (except static routes that explicitly configure a different table). Additionally, NetworkManager will not delete any extraneous routes from tables except the main table. This is to preserve backward compatibility for users who manage routing tables outside of NetworkManager.

    Format: uint32

ipv4.routes
    A list of IPv4 destination addresses, prefix length, optional IPv4 next hop addresses, optional route metric, optional attribute. The valid syntax is: "ip[/prefix] [next-hop] [metric] [attribute=val]...[,ip[/prefix]...]". For example "192.0.2.0/24 10.1.1.1 77, 198.51.100.0/24".

    Various attributes are supported:

        • "advmss" - an unsigned 32 bit integer.

        • "cwnd" - an unsigned 32 bit integer.

        • "initcwnd" - an unsigned 32 bit integer.

        • "initrwnd" - an unsigned 32 bit integer.

        • "lock-advmss" - a boolean value.

        • "lock-cwnd" - a boolean value.

        • "lock-initcwnd" - a boolean value.

        • "lock-initrwnd" - a boolean value.

        • "lock-mtu" - a boolean value.

        • "lock-window" - a boolean value.

        • "mtu" - an unsigned 32 bit integer.

        • "onlink" - a boolean value. The onlink flag is ignored for IPv4 routes without a gateway. That also means, with a positive "weight" the route cannot merge with ECMP routes which are onlink and have a gateway.

        • "quickack" - a boolean value.

        • "rto_min" - an unsigned 32 bit integer. The value is in milliseconds.

        • "scope" - an unsigned 8 bit integer. IPv4 only.

        • "src" - an IPv4 address.

        • "table" - an unsigned 32 bit integer. The default depends on ipv4.route-table.

        • "tos" - an unsigned 8 bit integer. IPv4 only.

        • "type" - one of unicast, local, blackhole, unreachable, prohibit, throw. The default is unicast.

        • "weight" - an unsigned 32 bit integer ranging from 0 to 256. A non-zero weight indicates that the IPv4 route is an ECMP IPv4 route. NetworkManager will automatically merge compatible ECMP routes into multi-hop routes. Setting to zero or omitting the attribute configures single hop routes that won't get merged. If the route finds no merge partner, it is configured as single hop route.

        Note that in NetworkManager, currently all nexthops of a ECMP route must share the same "onlink" flag in order to be mergable.

        • "window" - an unsigned 32 bit integer.

    For details see also `man ip-route`.

    Format: a comma separated list of routes

ipv4.routing-rules
    A comma separated list of routing rules for policy routing. The format is based on ip rule add syntax and mostly compatible. One difference is that routing rules in NetworkManager always need a fixed priority.

    Example: priority 5 from 192.167.4.0/24 table 45

    Format: a comma separated list of routing rules

  ipv6 setting

IPv6 Settings.

Properties:

ipv6.addr-gen-mode
    Configure method for creating the address for use with RFC4862 IPv6 Stateless Address Autoconfiguration. The permitted values are: NM_SETTING_IP6_CONFIG_ADDR_GEN_MODE_EUI64 (0), NM_SETTING_IP6_CONFIG_ADDR_GEN_MODE_STABLE_PRIVACY (1). NM_SETTING_IP6_CONFIG_ADDR_GEN_MODE_DEFAULT_OR_EUI64 (2) or NM_SETTING_IP6_CONFIG_ADDR_GEN_MODE_DEFAULT (3).

    If the property is set to EUI64, the addresses will be generated using the interface tokens derived from hardware address. This makes the host part of the address to stay constant, making it possible to track host's presence when it changes networks. The address changes when the interface hardware is replaced.

    The value of stable-privacy enables use of cryptographically secure hash of a secret host-specific key along with the connection's stable-id and the network address as specified by RFC7217. This makes it impossible to use the address track host's presence, and makes the address stable when the network interface hardware is replaced.

    The special values "default" and "default-or-eui64" will fallback to the global connection default in as documented in NetworkManager.conf(5) manual. If the global default is not specified, the fallback value is "stable-privacy" or "eui64", respectively.

    For libnm, the property defaults to "default" since 1.40. Previously it defaulted to "stable-privacy". On D-Bus, the absence of an addr-gen-mode setting equals "default". For keyfile plugin, the absence of the setting on disk means "default-or-eui64" so that the property doesn't change on upgrade from older versions.

    Note that this setting is distinct from the Privacy Extensions as configured by "ip6-privacy" property and it does not affect the temporary addresses configured with this option.

    Format: int32

ipv6.addresses
    Alias: ip6

    Array of IP addresses.

    Format: a comma separated list of addresses

ipv6.auto-route-ext-gw
    VPN connections will default to add the route automatically unless this setting is set to FALSE.

    For other connection types, adding such an automatic route is currently not supported and setting this to TRUE has no effect.

    Format: NMTernary (int32)

ipv6.dhcp-duid
    A string containing the DHCPv6 Unique Identifier (DUID) used by the dhcp client to identify itself to DHCPv6 servers (RFC 3315). The DUID is carried in the Client Identifier option. If the property is a hex string ('aa:bb:cc') it is interpreted as a binary DUID and filled as an opaque value in the Client Identifier option.

    The special value "lease" will retrieve the DUID previously used from the lease file belonging to the connection. If no DUID is found and "dhclient" is the configured dhcp client, the DUID is searched in the system-wide dhclient lease file. If still no DUID is found, or another dhcp client is used, a global and permanent DUID-UUID (RFC 6355) will be generated based on the machine-id.

    The special values "llt" and "ll" will generate a DUID of type LLT or LL (see RFC 3315) based on the current MAC address of the device. In order to try providing a stable DUID-LLT, the time field will contain a constant timestamp that is used globally (for all profiles) and persisted to disk.

    The special values "stable-llt", "stable-ll" and "stable-uuid" will generate a DUID of the corresponding type, derived from the connection's stable-id and a per-host unique key. You may want to include the "${DEVICE}" or "${MAC}" specifier in the stable-id, in case this profile gets activated on multiple devices. So, the link-layer address of "stable-ll" and "stable-llt" will be a generated address derived from the stable id. The DUID-LLT time value in the "stable-llt" option will be picked among a static timespan of three years (the upper bound of the interval is the same constant timestamp used in "llt").

    When the property is unset, the global value provided for "ipv6.dhcp-duid" is used. If no global value is provided, the default "lease" value is assumed.

    Format: string

ipv6.dhcp-hostname
    If the "dhcp-send-hostname" property is TRUE, then the specified name will be sent to the DHCP server when acquiring a lease. This property and "dhcp-fqdn" are mutually exclusive and cannot be set at the same time.

    Format: string

ipv6.dhcp-hostname-flags
    Flags for the DHCP hostname and FQDN.

    Currently, this property only includes flags to control the FQDN flags set in the DHCP FQDN option. Supported FQDN flags are NM_DHCP_HOSTNAME_FLAG_FQDN_SERV_UPDATE (0x1), NM_DHCP_HOSTNAME_FLAG_FQDN_ENCODED (0x2) and NM_DHCP_HOSTNAME_FLAG_FQDN_NO_UPDATE (0x4). When no FQDN flag is set and NM_DHCP_HOSTNAME_FLAG_FQDN_CLEAR_FLAGS (0x8) is set, the DHCP FQDN option will contain no flag. Otherwise, if no FQDN flag is set and NM_DHCP_HOSTNAME_FLAG_FQDN_CLEAR_FLAGS (0x8) is not set, the standard FQDN flags are set in the request: NM_DHCP_HOSTNAME_FLAG_FQDN_SERV_UPDATE (0x1), NM_DHCP_HOSTNAME_FLAG_FQDN_ENCODED (0x2) for IPv4 and NM_DHCP_HOSTNAME_FLAG_FQDN_SERV_UPDATE (0x1) for IPv6.

    When this property is set to the default value NM_DHCP_HOSTNAME_FLAG_NONE (0x0), a global default is looked up in NetworkManager configuration. If that value is unset or also NM_DHCP_HOSTNAME_FLAG_NONE (0x0), then the standard FQDN flags described above are sent in the DHCP requests.

    Format: uint32

ipv6.dhcp-iaid
    A string containing the "Identity Association Identifier" (IAID) used by the DHCP client. The string can be a 32-bit number (either decimal, hexadecimal or as colon separated hexadecimal numbers). Alternatively it can be set to the special values "mac", "perm-mac", "ifname" or "stable". When set to "mac" (or "perm-mac"), the last 4 bytes of the current (or permanent) MAC address are used as IAID. When set to "ifname", the IAID is computed by hashing the interface name. The special value "stable" can be used to generate an IAID based on the stable-id (see connection.stable-id), a per-host key and the interface name. When the property is unset, the value from global configuration is used; if no global default is set then the IAID is assumed to be "ifname".

    For DHCPv4, the IAID is only used with "ipv4.dhcp-client-id" values "duid" and "ipv6-duid" to generate the client-id.

    For DHCPv6, note that at the moment this property is only supported by the "internal" DHCPv6 plugin. The "dhclient" DHCPv6 plugin always derives the IAID from the MAC address.

    The actually used DHCPv6 IAID for a currently activated interface is exposed in the lease information of the device.

    Format: string

ipv6.dhcp-pd-hint
    A IPv6 address followed by a slash and a prefix length. If set, the value is sent to the DHCPv6 server as hint indicating the prefix delegation (IA_PD) we want to receive. To only hint a prefix length without prefix, set the address part to the zero address (for example "::/60").

    Format: string

ipv6.dhcp-send-hostname
    If TRUE, a hostname is sent to the DHCP server when acquiring a lease. Some DHCP servers use this hostname to update DNS databases, essentially providing a static hostname for the computer. If the "dhcp-hostname" property is NULL and this property is TRUE, the current persistent hostname of the computer is sent.

    Format: boolean

ipv6.dhcp-timeout
    A timeout for a DHCP transaction in seconds. If zero (the default), a globally configured default is used. If still unspecified, a device specific timeout is used (usually 45 seconds).

    Set to 2147483647 (MAXINT32) for infinity.

    Format: int32

ipv6.dns
    Array of IP addresses of DNS servers.

    For DoT (DNS over TLS), the SNI server name can be specified by appending "#example.com" to the IP address of the DNS server. This currently only has effect when using systemd-resolved.

    Format: array of byte array

ipv6.dns-options
    Array of DNS options as described in man 5 resolv.conf.

    NULL means that the options are unset and left at the default. In this case NetworkManager will use default options. This is distinct from an empty list of properties.

    The currently supported options are "attempts", "debug", "edns0", "inet6", "ip6-bytestring", "ip6-dotint", "ndots", "no-aaaa", "no-check-names", "no-ip6-dotint", "no-reload", "no-tld-query", "rotate", "single-request", "single-request-reopen", "timeout", "trust-ad", "use-vc".

    The "trust-ad" setting is only honored if the profile contributes name servers to resolv.conf, and if all contributing profiles have "trust-ad" enabled.

    When using a caching DNS plugin (dnsmasq or systemd-resolved in NetworkManager.conf) then "edns0" and "trust-ad" are automatically added.

    Format: array of string

ipv6.dns-priority
    DNS servers priority.

    The relative priority for DNS servers specified by this setting. A lower numerical value is better (higher priority).

    Negative values have the special effect of excluding other configurations with a greater numerical priority value; so in presence of at least one negative priority, only DNS servers from connections with the lowest priority value will be used. To avoid all DNS leaks, set the priority of the profile that should be used to the most negative value of all active connections profiles.

    Zero selects a globally configured default value. If the latter is missing or zero too, it defaults to 50 for VPNs (including WireGuard) and 100 for other connections.

    Note that the priority is to order DNS settings for multiple active connections. It does not disambiguate multiple DNS servers within the same connection profile.

    When multiple devices have configurations with the same priority, VPNs will be considered first, then devices with the best (lowest metric) default route and then all other devices.

    When using dns=default, servers with higher priority will be on top of resolv.conf. To prioritize a given server over another one within the same connection, just specify them in the desired order. Note that commonly the resolver tries name servers in /etc/resolv.conf in the order listed, proceeding with the next server in the list on failure. See for example the "rotate" option of the dns-options setting. If there are any negative DNS priorities, then only name servers from the devices with that lowest priority will be considered.

    When using a DNS resolver that supports Conditional Forwarding or Split DNS (with dns=dnsmasq or dns=systemd-resolved settings), each connection is used to query domains in its search list. The search domains determine which name servers to ask, and the DNS priority is used to prioritize name servers based on the domain. Queries for domains not present in any search list are routed through connections having the '~.' special wildcard domain, which is added automatically to connections with the default route (or can be added manually). When multiple connections specify the same domain, the one with the best priority (lowest numerical value) wins. If a sub domain is configured on another interface it will be accepted regardless the priority, unless parent domain on the other interface has a negative priority, which causes the sub domain to be shadowed. With Split DNS one can avoid undesired DNS leaks by properly configuring DNS priorities and the search domains, so that only name servers of the desired interface are configured.

    Format: int32

ipv6.dns-search
    List of DNS search domains. Domains starting with a tilde ('~') are considered 'routing' domains and are used only to decide the interface over which a query must be forwarded; they are not used to complete unqualified host names.

    When using a DNS plugin that supports Conditional Forwarding or Split DNS, then the search domains specify which name servers to query. This makes the behavior different from running with plain /etc/resolv.conf. For more information see also the dns-priority setting.

    When set on a profile that also enabled DHCP, the DNS search list received automatically (option 119 for DHCPv4 and option 24 for DHCPv6) gets merged with the manual list. This can be prevented by setting "ignore-auto-dns". Note that if no DNS searches are configured, the fallback will be derived from the domain from DHCP (option 15).

    Format: array of string

ipv6.gateway
    Alias: gw6

    The gateway associated with this configuration. This is only meaningful if "addresses" is also set.

    Setting the gateway causes NetworkManager to configure a standard default route with the gateway as next hop. This is ignored if "never-default" is set. An alternative is to configure the default route explicitly with a manual route and /0 as prefix length.

    Note that the gateway usually conflicts with routing that NetworkManager configures for WireGuard interfaces, so usually it should not be set in that case. See "ip4-auto-default-route".

    Format: string

ipv6.ignore-auto-dns
    When "method" is set to "auto" and this property to TRUE, automatically configured name servers and search domains are ignored and only name servers and search domains specified in the "dns" and "dns-search" properties, if any, are used.

    Format: boolean

ipv6.ignore-auto-routes
    When "method" is set to "auto" and this property to TRUE, automatically configured routes are ignored and only routes specified in the "routes" property, if any, are used.

    Format: boolean

ipv6.ip6-privacy
    Configure IPv6 Privacy Extensions for SLAAC, described in RFC4941. If enabled, it makes the kernel generate a temporary IPv6 address in addition to the public one generated from MAC address via modified EUI-64. This enhances privacy, but could cause problems in some applications, on the other hand. The permitted values are: -1: unknown, 0: disabled, 1: enabled (prefer public address), 2: enabled (prefer temporary addresses).

    Having a per-connection setting set to "-1" (unknown) means fallback to global configuration "ipv6.ip6-privacy".

    If also global configuration is unspecified or set to "-1", fallback to read "/proc/sys/net/ipv6/conf/default/use_tempaddr".

    Note that this setting is distinct from the Stable Privacy addresses that can be enabled with the "addr-gen-mode" property's "stable-privacy" setting as another way of avoiding host tracking with IPv6 addresses.

    Format: NMSettingIP6ConfigPrivacy (int32)

ipv6.may-fail
    If TRUE, allow overall network configuration to proceed even if the configuration specified by this property times out. Note that at least one IP configuration must succeed or overall network configuration will still fail. For example, in IPv6-only networks, setting this property to TRUE on the NMSettingIP4Config allows the overall network configuration to succeed if IPv4 configuration fails but IPv6 configuration completes successfully.

    Format: boolean

ipv6.method
    Sets the IPv6 connection method. You can set one of the following values:

        • "auto" - Enables IPv6 auto-configuration. By default, NetworkManager uses Router Advertisements and, if the router announces the "managed" flag, NetworkManager requests an IPv6 address and prefix from a DHCPv6 server.

        • "dhcp" - Requests an IPv6 address and prefix from a DHCPv6 server. Note that DHCPv6 does not have options to provide routes and the default gateway. As a consequence, by using the "dhcp" method, connections are limited to their own subnet.

        • "manual" - Enables the configuration of static IPv6 addresses on the interface. Note that you must set at least one IP address and prefix in the "ipv6.addresses" property.

        • "disabled" - Disables the IPv6 protocol in this connection profile.

        • "ignore" - Configures NetworkManager to make no changes to the IPv6 configuration on the interface. For example, you can then use the "accept_ra" feature of the kernel to accept Router Advertisements.

        • "shared" - Provides network access to other computers. NetworkManager requests a prefix from an upstream DHCPv6 server, assigns an address to the interface, and announces the prefix to clients that connect to this interface.

        • "link-local" - Assigns a random link-local address from the fe80::/64 subnet to the interface.

    If you set "auto", "dhcp", "manual", "ignore", or "shared", NetworkManager assigns, in addition to the global address, an IPv6 link-local address to the interface. This is compliant with RFC 4291.

    Format: string

ipv6.mtu
    Maximum transmission unit size, in bytes. If zero (the default), the MTU is set automatically from router advertisements or is left equal to the link-layer MTU. If greater than the link-layer MTU, or greater than zero but less than the minimum IPv6 MTU of 1280, this value has no effect.

    Format: uint32

ipv6.never-default
    If TRUE, this connection will never be the default connection for this IP type, meaning it will never be assigned the default route by NetworkManager.

    Format: boolean

ipv6.ra-timeout
    A timeout for waiting Router Advertisements in seconds. If zero (the default), a globally configured default is used. If still unspecified, the timeout depends on the sysctl settings of the device.

    Set to 2147483647 (MAXINT32) for infinity.

    Format: int32

ipv6.replace-local-rule
    Connections will default to keep the autogenerated priority 0 local rule unless this setting is set to TRUE.

    Format: NMTernary (int32)

ipv6.required-timeout
    The minimum time interval in milliseconds for which dynamic IP configuration should be tried before the connection succeeds.

    This property is useful for example if both IPv4 and IPv6 are enabled and are allowed to fail. Normally the connection succeeds as soon as one of the two address families completes; by setting a required timeout for e.g. IPv4, one can ensure that even if IP6 succeeds earlier than IPv4, NetworkManager waits some time for IPv4 before the connection becomes active.

    Note that if "may-fail" is FALSE for the same address family, this property has no effect as NetworkManager needs to wait for the full DHCP timeout.

    A zero value means that no required timeout is present, -1 means the default value (either configuration ipvx.required-timeout override or zero).

    Format: int32

ipv6.route-metric
    The default metric for routes that don't explicitly specify a metric. The default value -1 means that the metric is chosen automatically based on the device type. The metric applies to dynamic routes, manual (static) routes that don't have an explicit metric setting, address prefix routes, and the default route. Note that for IPv6, the kernel accepts zero (0) but coerces it to 1024 (user default). Hence, setting this property to zero effectively mean setting it to 1024. For IPv4, zero is a regular value for the metric.

    Format: int64

ipv6.route-table
    Enable policy routing (source routing) and set the routing table used when adding routes.

    This affects all routes, including device-routes, IPv4LL, DHCP, SLAAC, default-routes and static routes. But note that static routes can individually overwrite the setting by explicitly specifying a non-zero routing table.

    If the table setting is left at zero, it is eligible to be overwritten via global configuration. If the property is zero even after applying the global configuration value, policy routing is disabled for the address family of this connection.

    Policy routing disabled means that NetworkManager will add all routes to the main table (except static routes that explicitly configure a different table). Additionally, NetworkManager will not delete any extraneous routes from tables except the main table. This is to preserve backward compatibility for users who manage routing tables outside of NetworkManager.

    Format: uint32

ipv6.routes
    A list of IPv6 destination addresses, prefix length, optional IPv6 next hop addresses, optional route metric, optional attribute. The valid syntax is: "ip[/prefix] [next-hop] [metric] [attribute=val]...[,ip[/prefix]...]".

    Various attributes are supported:

        • "advmss" - an unsigned 32 bit integer.

        • "cwnd" - an unsigned 32 bit integer.

        • "from" - an IPv6 address with optional prefix. IPv6 only.

        • "initcwnd" - an unsigned 32 bit integer.

        • "initrwnd" - an unsigned 32 bit integer.

        • "lock-advmss" - a boolean value.

        • "lock-cwnd" - a boolean value.

        • "lock-initcwnd" - a boolean value.

        • "lock-initrwnd" - a boolean value.

        • "lock-mtu" - a boolean value.

        • "lock-window" - a boolean value.

        • "mtu" - an unsigned 32 bit integer.

        • "onlink" - a boolean value.

        • "quickack" - a boolean value.

        • "rto_min" - an unsigned 32 bit integer. The value is in milliseconds.

        • "src" - an IPv6 address.

        • "table" - an unsigned 32 bit integer. The default depends on ipv6.route-table.

        • "type" - one of unicast, local, blackhole, unreachable, prohibit, throw. The default is unicast.

        • "window" - an unsigned 32 bit integer.

    For details see also `man ip-route`.

    Format: a comma separated list of routes

ipv6.routing-rules
    A comma separated list of routing rules for policy routing. The format is based on ip rule add syntax and mostly compatible. One difference is that routing rules in NetworkManager always need a fixed priority.

    Example: priority 5 from 1:2:3::5/128 table 45

    Format: a comma separated list of routing rules

ipv6.token
    Configure the token for draft-chown-6man-tokenised-ipv6-identifiers-02 IPv6 tokenized interface identifiers. Useful with eui64 addr-gen-mode.

    Format: string

  ip-tunnel setting

IP Tunneling Settings.

Properties:

ip-tunnel.encapsulation-limit
    How many additional levels of encapsulation are permitted to be prepended to packets. This property applies only to IPv6 tunnels. To disable this option, add NM_IP_TUNNEL_FLAG_IP6_IGN_ENCAP_LIMIT (0x1) to ip-tunnel flags.

    Format: uint32

ip-tunnel.flags
    Tunnel flags. Currently, the following values are supported: NM_IP_TUNNEL_FLAG_IP6_IGN_ENCAP_LIMIT (0x1), NM_IP_TUNNEL_FLAG_IP6_USE_ORIG_TCLASS (0x2), NM_IP_TUNNEL_FLAG_IP6_USE_ORIG_FLOWLABEL (0x4), NM_IP_TUNNEL_FLAG_IP6_MIP6_DEV (0x8), NM_IP_TUNNEL_FLAG_IP6_RCV_DSCP_COPY (0x10), NM_IP_TUNNEL_FLAG_IP6_USE_ORIG_FWMARK (0x20). They are valid only for IPv6 tunnels.

    Format: uint32

ip-tunnel.flow-label
    The flow label to assign to tunnel packets. This property applies only to IPv6 tunnels.

    Format: uint32

ip-tunnel.fwmark
    The fwmark value to assign to tunnel packets. This property can be set to a non zero value only on VTI and VTI6 tunnels.

    Format: uint32

ip-tunnel.input-key
    The key used for tunnel input packets; the property is valid only for certain tunnel modes (GRE, IP6GRE). If empty, no key is used.

    Format: string

ip-tunnel.local
    Alias: local

    The local endpoint of the tunnel; the value can be empty, otherwise it must contain an IPv4 or IPv6 address.

    Format: string

ip-tunnel.mode
    Alias: mode

    The tunneling mode, for example NM_IP_TUNNEL_MODE_IPIP (1) or NM_IP_TUNNEL_MODE_GRE (2).

    Format: uint32

ip-tunnel.mtu
    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple fragments.

    Format: uint32

ip-tunnel.output-key
    The key used for tunnel output packets; the property is valid only for certain tunnel modes (GRE, IP6GRE). If empty, no key is used.

    Format: string

ip-tunnel.parent
    Alias: dev

    If given, specifies the parent interface name or parent connection UUID the new device will be bound to so that tunneled packets will only be routed via that interface.

    Format: string

ip-tunnel.path-mtu-discovery
    Whether to enable Path MTU Discovery on this tunnel.

    Format: boolean

ip-tunnel.remote
    Alias: remote

    The remote endpoint of the tunnel; the value must contain an IPv4 or IPv6 address.

    Format: string

ip-tunnel.tos
    The type of service (IPv4) or traffic class (IPv6) field to be set on tunneled packets.

    Format: uint32

ip-tunnel.ttl
    The TTL to assign to tunneled packets. 0 is a special value meaning that packets inherit the TTL value.

    Format: uint32

  macsec setting

MACSec Settings.

Properties:

macsec.encrypt
    Alias: encrypt

    Whether the transmitted traffic must be encrypted.

    Format: boolean

macsec.mka-cak
    Alias: cak

    The pre-shared CAK (Connectivity Association Key) for MACsec Key Agreement. Must be a string of 32 hexadecimal characters.

    Format: string

macsec.mka-cak-flags
    Flags indicating how to handle the "mka-cak" property.

    Format: NMSettingSecretFlags (uint32)

macsec.mka-ckn
    Alias: ckn

    The pre-shared CKN (Connectivity-association Key Name) for MACsec Key Agreement. Must be a string of hexadecimal characters with a even length between 2 and 64.

    Format: string

macsec.mode
    Alias: mode

    Specifies how the CAK (Connectivity Association Key) for MKA (MACsec Key Agreement) is obtained.

    Format: int32

macsec.parent
    Alias: dev

    If given, specifies the parent interface name or parent connection UUID from which this MACSEC interface should be created. If this property is not specified, the connection must contain an "802-3-ethernet" setting with a "mac-address" property.

    Format: string

macsec.port
    Alias: port

    The port component of the SCI (Secure Channel Identifier), between 1 and 65534.

    Format: int32

macsec.send-sci
    Specifies whether the SCI (Secure Channel Identifier) is included in every packet.

    Format: boolean

macsec.validation
    Specifies the validation mode for incoming frames.

    Format: int32

  macvlan setting

MAC VLAN Settings.

Properties:

macvlan.mode
    Alias: mode

    The macvlan mode, which specifies the communication mechanism between multiple macvlans on the same lower device.

    Format: uint32

macvlan.parent
    Alias: dev

    If given, specifies the parent interface name or parent connection UUID from which this MAC-VLAN interface should be created. If this property is not specified, the connection must contain an "802-3-ethernet" setting with a "mac-address" property.

    Format: string

macvlan.promiscuous
    Whether the interface should be put in promiscuous mode.

    Format: boolean

macvlan.tap
    Alias: tap

    Whether the interface should be a MACVTAP.

    Format: boolean

  match setting

Match settings.

Properties:

match.driver
    A list of driver names to match. Each element is a shell wildcard pattern.

    See NMSettingMatch:interface-name for how special characters '|', '&', '!' and '\\' are used for optional and mandatory matches and inverting the pattern.

    Format: array of string

match.interface-name
    A list of interface names to match. Each element is a shell wildcard pattern.

    An element can be prefixed with a pipe symbol (|) or an ampersand (&). The former means that the element is optional and the latter means that it is mandatory. If there are any optional elements, than the match evaluates to true if at least one of the optional element matches (logical OR). If there are any mandatory elements, then they all must match (logical AND). By default, an element is optional. This means that an element "foo" behaves the same as "|foo". An element can also be inverted with exclamation mark (!) between the pipe symbol (or the ampersand) and before the pattern. Note that "!foo" is a shortcut for the mandatory match "&!foo". Finally, a backslash can be used at the beginning of the element (after the optional special characters) to escape the start of the pattern. For example, "&\\!a" is an mandatory match for literally "!a".

    Format: array of string

match.kernel-command-line
    A list of kernel command line arguments to match. This may be used to check whether a specific kernel command line option is set (or unset, if prefixed with the exclamation mark). The argument must either be a single word, or an assignment (i.e. two words, joined by "="). In the former case the kernel command line is searched for the word appearing as is, or as left hand side of an assignment. In the latter case, the exact assignment is looked for with right and left hand side matching. Wildcard patterns are not supported.

    See NMSettingMatch:interface-name for how special characters '|', '&', '!' and '\\' are used for optional and mandatory matches and inverting the match.

    Format: array of string

match.path
    A list of paths to match against the ID_PATH udev property of devices. ID_PATH represents the topological persistent path of a device. It typically contains a subsystem string (pci, usb, platform, etc.) and a subsystem-specific identifier.

    For PCI devices the path has the form "pci-$domain:$bus:$device.$function", where each variable is an hexadecimal value; for example "pci-0000:0a:00.0".

    The path of a device can be obtained with "udevadm info /sys/class/net/$dev | grep ID_PATH=" or by looking at the "path" property exported by NetworkManager ("nmcli -f general.path device show $dev").

    Each element of the list is a shell wildcard pattern.

    See NMSettingMatch:interface-name for how special characters '|', '&', '!' and '\\' are used for optional and mandatory matches and inverting the pattern.

    Format: array of string

  802-11-olpc-mesh setting

Alias: olpc-mesh

OLPC Wireless Mesh Settings.

Properties:

802-11-olpc-mesh.channel
    Alias: channel

    Channel on which the mesh network to join is located.

    Format: uint32

802-11-olpc-mesh.dhcp-anycast-address
    Alias: dhcp-anycast

    Anycast DHCP MAC address used when requesting an IP address via DHCP. The specific anycast address used determines which DHCP server class answers the request.

    This is currently only implemented by dhclient DHCP plugin.

    Format: byte array

802-11-olpc-mesh.ssid
    Alias: ssid

    SSID of the mesh network to join.

    Format: byte array

  ovs-bridge setting

OvsBridge Link Settings.

Properties:

ovs-bridge.datapath-type
    The data path type. One of "system", "netdev" or empty.

    Format: string

ovs-bridge.fail-mode
    The bridge failure mode. One of "secure", "standalone" or empty.

    Format: string

ovs-bridge.mcast-snooping-enable
    Enable or disable multicast snooping.

    Format: boolean

ovs-bridge.rstp-enable
    Enable or disable RSTP.

    Format: boolean

ovs-bridge.stp-enable
    Enable or disable STP.

    Format: boolean

  ovs-dpdk setting

OvsDpdk Link Settings.

Properties:

ovs-dpdk.devargs
    Open vSwitch DPDK device arguments.

    Format: string

ovs-dpdk.n-rxq
    Open vSwitch DPDK number of rx queues. Defaults to zero which means to leave the parameter in OVS unspecified and effectively configures one queue.

    Format: uint32

ovs-dpdk.n-rxq-desc
    The rx queue size (number of rx descriptors) for DPDK ports. Must be zero or a power of 2 between 1 and 4096, and supported by the hardware. Defaults to zero which means to leave the parameter in OVS unspecified and effectively configures 2048 descriptors.

    Format: uint32

ovs-dpdk.n-txq-desc
    The tx queue size (number of tx descriptors) for DPDK ports. Must be zero or a power of 2 between 1 and 4096, and supported by the hardware. Defaults to zero which means to leave the parameter in OVS unspecified and effectively configures 2048 descriptors.

    Format: uint32

  ovs-interface setting

Open vSwitch Interface Settings.

Properties:

ovs-interface.ofport-request
    Open vSwitch openflow port number. Defaults to zero which means that port number will not be specified and it will be chosen randomly by ovs. OpenFlow ports are the network interfaces for passing packets between OpenFlow processing and the rest of the network. OpenFlow switches connect logically to each other via their OpenFlow ports.

    Format: uint32

ovs-interface.type
    The interface type. Either "internal", "system", "patch", "dpdk", or empty.

    Format: string

  ovs-patch setting

OvsPatch Link Settings.

Properties:

ovs-patch.peer
    Specifies the name of the interface for the other side of the patch. The patch on the other side must also set this interface as peer.

    Format: string

  ovs-port setting

OvsPort Link Settings.

Properties:

ovs-port.bond-downdelay
    The time port must be inactive in order to be considered down.

    Format: uint32

ovs-port.bond-mode
    Bonding mode. One of "active-backup", "balance-slb", or "balance-tcp".

    Format: string

ovs-port.bond-updelay
    The time port must be active before it starts forwarding traffic.

    Format: uint32

ovs-port.lacp
    LACP mode. One of "active", "off", or "passive".

    Format: string

ovs-port.tag
    The VLAN tag in the range 0-4095.

    Format: uint32

ovs-port.trunks
    A list of VLAN ranges that this port trunks.

    The property is valid only for ports with mode "trunk", "native-tagged", or "native-untagged port". If it is empty, the port trunks all VLANs.

    Format: array of vardict

ovs-port.vlan-mode
    The VLAN mode. One of "access", "native-tagged", "native-untagged", "trunk", "dot1q-tunnel" or unset.

    Format: string

  ppp setting

Point-to-Point Protocol Settings.

Properties:

ppp.baud
    If non-zero, instruct pppd to set the serial port to the specified baudrate. This value should normally be left as 0 to automatically choose the speed.

    Format: uint32

ppp.crtscts
    If TRUE, specify that pppd should set the serial port to use hardware flow control with RTS and CTS signals. This value should normally be set to FALSE.

    Format: boolean

ppp.lcp-echo-failure
    If non-zero, instruct pppd to presume the connection to the peer has failed if the specified number of LCP echo-requests go unanswered by the peer. The "lcp-echo-interval" property must also be set to a non-zero value if this property is used.

    Format: uint32

ppp.lcp-echo-interval
    If non-zero, instruct pppd to send an LCP echo-request frame to the peer every n seconds (where n is the specified value). Note that some PPP peers will respond to echo requests and some will not, and it is not possible to autodetect this.

    Format: uint32

ppp.mppe-stateful
    If TRUE, stateful MPPE is used. See pppd documentation for more information on stateful MPPE.

    Format: boolean

ppp.mru
    If non-zero, instruct pppd to request that the peer send packets no larger than the specified size. If non-zero, the MRU should be between 128 and 16384.

    Format: uint32

ppp.mtu
    If non-zero, instruct pppd to send packets no larger than the specified size.

    Format: uint32

ppp.no-vj-comp
    If TRUE, Van Jacobsen TCP header compression will not be requested.

    Format: boolean

ppp.noauth
    If TRUE, do not require the other side (usually the PPP server) to authenticate itself to the client. If FALSE, require authentication from the remote side. In almost all cases, this should be TRUE.

    Format: boolean

ppp.nobsdcomp
    If TRUE, BSD compression will not be requested.

    Format: boolean

ppp.nodeflate
    If TRUE, "deflate" compression will not be requested.

    Format: boolean

ppp.refuse-chap
    If TRUE, the CHAP authentication method will not be used.

    Format: boolean

ppp.refuse-eap
    If TRUE, the EAP authentication method will not be used.

    Format: boolean

ppp.refuse-mschap
    If TRUE, the MSCHAP authentication method will not be used.

    Format: boolean

ppp.refuse-mschapv2
    If TRUE, the MSCHAPv2 authentication method will not be used.

    Format: boolean

ppp.refuse-pap
    If TRUE, the PAP authentication method will not be used.

    Format: boolean

ppp.require-mppe
    If TRUE, MPPE (Microsoft Point-to-Point Encryption) will be required for the PPP session. If either 64-bit or 128-bit MPPE is not available the session will fail. Note that MPPE is not used on mobile broadband connections.

    Format: boolean

ppp.require-mppe-128
    If TRUE, 128-bit MPPE (Microsoft Point-to-Point Encryption) will be required for the PPP session, and the "require-mppe" property must also be set to TRUE. If 128-bit MPPE is not available the session will fail.

    Format: boolean

  pppoe setting

PPP-over-Ethernet Settings.

Properties:

pppoe.parent
    Alias: parent

    If given, specifies the parent interface name on which this PPPoE connection should be created. If this property is not specified, the connection is activated on the interface specified in "interface-name" of NMSettingConnection.

    Format: string

pppoe.password
    Alias: password

    Password used to authenticate with the PPPoE service.

    Format: string

pppoe.password-flags
    Flags indicating how to handle the "password" property.

    Format: NMSettingSecretFlags (uint32)

pppoe.service
    Alias: service

    If specified, instruct PPPoE to only initiate sessions with access concentrators that provide the specified service. For most providers, this should be left blank. It is only required if there are multiple access concentrators or a specific service is known to be required.

    Format: string

pppoe.username
    Alias: username

    Username used to authenticate with the PPPoE service.

    Format: string

  proxy setting

WWW Proxy Settings.

Properties:

proxy.browser-only
    Alias: browser-only

    Whether the proxy configuration is for browser only.

    Format: boolean

proxy.method
    Alias: method

    Method for proxy configuration, Default is NM_SETTING_PROXY_METHOD_NONE (0)

    Format: int32

proxy.pac-script
    Alias: pac-script

    PAC script for the connection. This is an UTF-8 encoded javascript code that defines a FindProxyForURL() function.

    Format: string

proxy.pac-url
    Alias: pac-url

    PAC URL for obtaining PAC file.

    Format: string

  serial setting

Serial Link Settings.

Properties:

serial.baud
    Speed to use for communication over the serial port. Note that this value usually has no effect for mobile broadband modems as they generally ignore speed settings and use the highest available speed.

    Format: uint32

serial.bits
    Byte-width of the serial communication. The 8 in "8n1" for example.

    Format: uint32

serial.parity
    Parity setting of the serial port.

    Format: NMSettingSerialParity (byte)

serial.send-delay
    Time to delay between each byte sent to the modem, in microseconds.

    Format: uint64

serial.stopbits
    Number of stop bits for communication on the serial port. Either 1 or 2. The 1 in "8n1" for example.

    Format: uint32

  sriov setting

SR-IOV settings.

Properties:

sriov.autoprobe-drivers
    Whether to autoprobe virtual functions by a compatible driver.

    If set to NM_TERNARY_TRUE (1), the kernel will try to bind VFs to a compatible driver and if this succeeds a new network interface will be instantiated for each VF.

    If set to NM_TERNARY_FALSE (0), VFs will not be claimed and no network interfaces will be created for them.

    When set to NM_TERNARY_DEFAULT (-1), the global default is used; in case the global default is unspecified it is assumed to be NM_TERNARY_TRUE (1).

    Format: NMTernary (int32)

sriov.total-vfs
    The total number of virtual functions to create.

    Note that when the sriov setting is present NetworkManager enforces the number of virtual functions on the interface (also when it is zero) during activation and resets it upon deactivation. To prevent any changes to SR-IOV parameters don't add a sriov setting to the connection.

    Format: uint32

sriov.vfs
    Array of virtual function descriptors.

    Each VF descriptor is a dictionary mapping attribute names to GVariant values. The 'index' entry is mandatory for each VF.

    When represented as string a VF is in the form:

    "INDEX [ATTR=VALUE[ ATTR=VALUE]...]".

    for example:

    "2 mac=00:11:22:33:44:55 spoof-check=true".

    Multiple VFs can be specified using a comma as separator. Currently, the following attributes are supported: mac, spoof-check, trust, min-tx-rate, max-tx-rate, vlans.

    The "vlans" attribute is represented as a semicolon-separated list of VLAN descriptors, where each descriptor has the form

    "ID[.PRIORITY[.PROTO]]".

    PROTO can be either 'q' for 802.1Q (the default) or 'ad' for 802.1ad.

    Format: array of vardict

  tc setting

Linux Traffic Control Settings.

Properties:

tc.qdiscs
    Array of TC queueing disciplines. qdisc is a basic block in the Linux traffic control subsystem

    Each qdisc can be specified by the following attributes:

    handle HANDLE
        specifies the qdisc handle. A qdisc, which potentially can have children, gets assigned a major number, called a 'handle', leaving the minor number namespace available for classes. The handle is expressed as '10:'. It is customary to explicitly assign a handle to qdiscs expected to have children.

    parent HANDLE
        specifies the handle of the parent qdisc the current qdisc must be attached to.

    root
        specifies that the qdisc is attached to the root of device.

    KIND
        this is the qdisc kind. NetworkManager currently supports the following kinds: fq_codel, sfq, tbf. Each qdisc kind has a different set of parameters, described below. There are also some kinds like pfifo, pfifo_fast, prio supported by NetworkManager but their parameters are not supported by NetworkManager.

    Parameters for 'fq_codel':

    limit U32
        the hard limit on the real queue size. When this limit is reached, incoming packets are dropped. Default is 10240 packets.

    memory_limit U32
        sets a limit on the total number of bytes that can be queued in this FQ-CoDel instance. The lower of the packet limit of the limit parameter and the memory limit will be enforced. Default is 32 MB.

    flows U32
        the number of flows into which the incoming packets are classified. Due to the stochastic nature of hashing, multiple flows may end up being hashed into the same slot. Newer flows have priority over older ones. This parameter can be set only at load time since memory has to be allocated for the hash table. Default value is 1024.

    target U32
        the acceptable minimum standing/persistent queue delay. This minimum delay is identified by tracking the local minimum queue delay that packets experience. The unit of measurement is microsecond(us). Default value is 5ms.

    interval U32
        used to ensure that the measured minimum delay does not become too stale. The minimum delay must be experienced in the last epoch of length .B interval. It should be set on the order of the worst-case RTT through the bottleneck to give endpoints sufficient time to react. Default value is 100ms.

    quantum U32
        the number of bytes used as 'deficit' in the fair queuing algorithm. Default is set to 1514 bytes which corresponds to the Ethernet MTU plus the hardware header length of 14 bytes.

    ecn BOOL
        can be used to mark packets instead of dropping them. ecn is turned on by default.

    ce_threshold U32
        sets a threshold above which all packets are marked with ECN Congestion Experienced. This is useful for DCTCP-style congestion control algorithms that require marking at very shallow queueing thresholds.

    Parameters for 'sfq':

    divisor U32
        can be used to set a different hash table size, available from kernel 2.6.39 onwards. The specified divisor must be a power of two and cannot be larger than 65536. Default value: 1024.

    limit U32
        Upper limit of the SFQ. Can be used to reduce the default length of 127 packets.

    depth U32
        Limit of packets per flow. Default to 127 and can be lowered.

    perturb_period U32
        Interval in seconds for queue algorithm perturbation. Defaults to 0, which means that no perturbation occurs. Do not set too low for each perturbation may cause some packet reordering or losses. Advised value: 60 This value has no effect when external flow classification is used. Its better to increase divisor value to lower risk of hash collisions.

    quantum U32
        Amount of bytes a flow is allowed to dequeue during a round of the round robin process. Defaults to the MTU of the interface which is also the advised value and the minimum value.

    flows U32
        Default value is 127.

    Parameters for 'tbf':

    rate U64
        Bandwidth or rate. These parameters accept a floating point number, possibly followed by either a unit (both SI and IEC units supported), or a float followed by a percent character to specify the rate as a percentage of the device's speed.

    burst U32
        Also known as buffer or maxburst. Size of the bucket, in bytes. This is the maximum amount of bytes that tokens can be available for instantaneously. In general, larger shaping rates require a larger buffer. For 10mbit/s on Intel, you need at least 10kbyte buffer if you want to reach your configured rate!

        If your buffer is too small, packets may be dropped because more tokens arrive per timer tick than fit in your bucket. The minimum buffer size can be calculated by dividing the rate by HZ.

        Token usage calculations are performed using a table which by default has a resolution of 8 packets. This resolution can be changed by specifying the cell size with the burst. For example, to specify a 6000 byte buffer with a 16 byte cell size, set a burst of 6000/16. You will probably never have to set this. Must be an integral power of 2.

    limit U32
        Limit is the number of bytes that can be queued waiting for tokens to become available.

    latency U32
        specifies the maximum amount of time a packet can sit in the TBF. The latency calculation takes into account the size of the bucket, the rate and possibly the peakrate (if set). The latency and limit are mutually exclusive.

    Format: GPtrArray(NMTCQdisc)

tc.tfilters
    Array of TC traffic filters. Traffic control can manage the packet content during classification by using filters.

    Each tfilters can be specified by the following attributes:

    handle HANDLE
        specifies the tfilters handle. A filter is used by a classful qdisc to determine in which class a packet will be enqueued. It is important to notice that filters reside within qdiscs. Therefore, see qdiscs handle for detailed information.

    parent HANDLE
        specifies the handle of the parent qdisc the current qdisc must be attached to.

    root
        specifies that the qdisc is attached to the root of device.

    KIND
        this is the tfilters kind. NetworkManager currently supports following kinds: mirred, simple. Each filter kind has a different set of actions, described below. There are also some other kinds like matchall, basic, u32 supported by NetworkManager.

    Actions for 'mirred':

    egress bool
        Define whether the packet should exit from the interface.

    ingress bool
        Define whether the packet should come into the interface.

    mirror bool
        Define whether the packet should be copied to the destination space.

    redirect bool
        Define whether the packet should be moved to the destination space.

    Action for 'simple':

    sdata char[32]
        The actual string to print.

    Format: GPtrArray(NMTCTfilter)

  team setting

Teaming Settings.

Properties:

team.config
    Alias: config

    The JSON configuration for the team network interface. The property should contain raw JSON configuration data suitable for teamd, because the value is passed directly to teamd. If not specified, the default configuration is used. See man teamd.conf for the format details.

    Format: string

team.link-watchers
    Link watchers configuration for the connection: each link watcher is defined by a dictionary, whose keys depend upon the selected link watcher. Available link watchers are 'ethtool', 'nsna_ping' and 'arp_ping' and it is specified in the dictionary with the key 'name'. Available keys are: ethtool: 'delay-up', 'delay-down', 'init-wait'; nsna_ping: 'init-wait', 'interval', 'missed-max', 'target-host'; arp_ping: all the ones in nsna_ping and 'source-host', 'validate-active', 'validate-inactive', 'send-always'. See teamd.conf man for more details.

    Format: array of vardict

team.mcast-rejoin-count
    Corresponds to the teamd mcast_rejoin.count.

    Format: int32

team.mcast-rejoin-interval
    Corresponds to the teamd mcast_rejoin.interval.

    Format: int32

team.notify-peers-count
    Corresponds to the teamd notify_peers.count.

    Format: int32

team.notify-peers-interval
    Corresponds to the teamd notify_peers.interval.

    Format: int32

team.runner
    Corresponds to the teamd runner.name. Permitted values are: "roundrobin", "broadcast", "activebackup", "loadbalance", "lacp", "random".

    Format: string

team.runner-active
    Corresponds to the teamd runner.active.

    Format: boolean

team.runner-agg-select-policy
    Corresponds to the teamd runner.agg_select_policy.

    Format: string

team.runner-fast-rate
    Corresponds to the teamd runner.fast_rate.

    Format: boolean

team.runner-hwaddr-policy
    Corresponds to the teamd runner.hwaddr_policy.

    Format: string

team.runner-min-ports
    Corresponds to the teamd runner.min_ports.

    Format: int32

team.runner-sys-prio
    Corresponds to the teamd runner.sys_prio.

    Format: int32

team.runner-tx-balancer
    Corresponds to the teamd runner.tx_balancer.name.

    Format: string

team.runner-tx-balancer-interval
    Corresponds to the teamd runner.tx_balancer.interval.

    Format: int32

team.runner-tx-hash
    Corresponds to the teamd runner.tx_hash.

    Format: array of string

  team-port setting

Team Port Settings.

Properties:

team-port.config
    Alias: config

    The JSON configuration for the team port. The property should contain raw JSON configuration data suitable for teamd, because the value is passed directly to teamd. If not specified, the default configuration is used. See man teamd.conf for the format details.

    Format: string

team-port.lacp-key
    Corresponds to the teamd ports.PORTIFNAME.lacp_key.

    Format: int32

team-port.lacp-prio
    Corresponds to the teamd ports.PORTIFNAME.lacp_prio.

    Format: int32

team-port.link-watchers
    Link watchers configuration for the connection: each link watcher is defined by a dictionary, whose keys depend upon the selected link watcher. Available link watchers are 'ethtool', 'nsna_ping' and 'arp_ping' and it is specified in the dictionary with the key 'name'. Available keys are: ethtool: 'delay-up', 'delay-down', 'init-wait'; nsna_ping: 'init-wait', 'interval', 'missed-max', 'target-host'; arp_ping: all the ones in nsna_ping and 'source-host', 'validate-active', 'validate-inactive', 'send-always'. See teamd.conf man for more details.

    Format: array of vardict

team-port.prio
    Corresponds to the teamd ports.PORTIFNAME.prio.

    Format: int32

team-port.queue-id
    Corresponds to the teamd ports.PORTIFNAME.queue_id. When set to -1 means the parameter is skipped from the json config.

    Format: int32

team-port.sticky
    Corresponds to the teamd ports.PORTIFNAME.sticky.

    Format: boolean

  tun setting

Tunnel Settings.

Properties:

tun.group
    Alias: group

    The group ID which will own the device. If set to NULL everyone will be able to use the device.

    Format: string

tun.mode
    Alias: mode

    The operating mode of the virtual device. Allowed values are NM_SETTING_TUN_MODE_TUN (1) to create a layer 3 device and NM_SETTING_TUN_MODE_TAP (2) to create an Ethernet-like layer 2 one.

    Format: uint32

tun.multi-queue
    Alias: multi-queue

    If the property is set to TRUE, the interface will support multiple file descriptors (queues) to parallelize packet sending or receiving. Otherwise, the interface will only support a single queue.

    Format: boolean

tun.owner
    Alias: owner

    The user ID which will own the device. If set to NULL everyone will be able to use the device.

    Format: string

tun.pi
    Alias: pi

    If TRUE the interface will prepend a 4 byte header describing the physical interface to the packets.

    Format: boolean

tun.vnet-hdr
    Alias: vnet-hdr

    If TRUE the IFF_VNET_HDR the tunnel packets will include a virtio network header.

    Format: boolean

  vlan setting

VLAN Settings.

Properties:

vlan.egress-priority-map
    Alias: egress

    For outgoing packets, a list of mappings from Linux SKB priorities to 802.1p priorities. The mapping is given in the format "from:to" where both "from" and "to" are unsigned integers, ie "7:3".

    Format: array of string

vlan.flags
    Alias: flags

    One or more flags which control the behavior and features of the VLAN interface. Flags include NM_VLAN_FLAG_REORDER_HEADERS (0x1) (reordering of output packet headers), NM_VLAN_FLAG_GVRP (0x2) (use of the GVRP protocol), and NM_VLAN_FLAG_LOOSE_BINDING (0x4) (loose binding of the interface to its master device's operating state). NM_VLAN_FLAG_MVRP (0x8) (use of the MVRP protocol).

    The default value of this property is NM_VLAN_FLAG_REORDER_HEADERS, but it used to be 0. To preserve backward compatibility, the default-value in the D-Bus API continues to be 0 and a missing property on D-Bus is still considered as 0.

    Format: NMVlanFlags (uint32)

vlan.id
    Alias: id

    The VLAN identifier that the interface created by this connection should be assigned. The valid range is from 0 to 4094, without the reserved id 4095.

    Format: uint32

vlan.ingress-priority-map
    Alias: ingress

    For incoming packets, a list of mappings from 802.1p priorities to Linux SKB priorities. The mapping is given in the format "from:to" where both "from" and "to" are unsigned integers, ie "7:3".

    Format: array of string

vlan.parent
    Alias: dev

    If given, specifies the parent interface name or parent connection UUID from which this VLAN interface should be created. If this property is not specified, the connection must contain an "802-3-ethernet" setting with a "mac-address" property.

    Format: string

vlan.protocol
    Specifies the VLAN protocol to use for encapsulation.

    Supported values are: '802.1Q', '802.1ad'. If not specified the default value is '802.1Q'.

    Format: string

  vpn setting

VPN Settings.

Properties:

vpn.data
    Dictionary of key/value pairs of VPN plugin specific data. Both keys and values must be strings.

    Format: dict of string to string

vpn.persistent
    If the VPN service supports persistence, and this property is TRUE, the VPN will attempt to stay connected across link changes and outages, until explicitly disconnected.

    Format: boolean

vpn.secrets
    Dictionary of key/value pairs of VPN plugin specific secrets like passwords or private keys. Both keys and values must be strings.

    Format: dict of string to string

vpn.service-type
    Alias: vpn-type

    D-Bus service name of the VPN plugin that this setting uses to connect to its network. i.e. org.freedesktop.NetworkManager.vpnc for the vpnc plugin.

    Format: string

vpn.timeout
    Timeout for the VPN service to establish the connection. Some services may take quite a long time to connect. Value of 0 means a default timeout, which is 60 seconds (unless overridden by vpn.timeout in configuration file). Values greater than zero mean timeout in seconds.

    Format: uint32

vpn.user-name
    Alias: user

    If the VPN connection requires a user name for authentication, that name should be provided here. If the connection is available to more than one user, and the VPN requires each user to supply a different name, then leave this property empty. If this property is empty, NetworkManager will automatically supply the username of the user which requested the VPN connection.

    Format: string

  vrf setting

VRF settings.

Properties:

vrf.table
    Alias: table

    The routing table for this VRF.

    Format: uint32

  vxlan setting

VXLAN Settings.

Properties:

vxlan.ageing
    Specifies the lifetime in seconds of FDB entries learnt by the kernel.

    Format: uint32

vxlan.destination-port
    Alias: destination-port

    Specifies the UDP destination port to communicate to the remote VXLAN tunnel endpoint.

    Format: uint32

vxlan.id
    Alias: id

    Specifies the VXLAN Network Identifier (or VXLAN Segment Identifier) to use.

    Format: uint32

vxlan.l2-miss
    Specifies whether netlink LL ADDR miss notifications are generated.

    Format: boolean

vxlan.l3-miss
    Specifies whether netlink IP ADDR miss notifications are generated.

    Format: boolean

vxlan.learning
    Specifies whether unknown source link layer addresses and IP addresses are entered into the VXLAN device forwarding database.

    Format: boolean

vxlan.limit
    Specifies the maximum number of FDB entries. A value of zero means that the kernel will store unlimited entries.

    Format: uint32

vxlan.local
    Alias: local

    If given, specifies the source IP address to use in outgoing packets.

    Format: string

vxlan.parent
    Alias: dev

    If given, specifies the parent interface name or parent connection UUID.

    Format: string

vxlan.proxy
    Specifies whether ARP proxy is turned on.

    Format: boolean

vxlan.remote
    Alias: remote

    Specifies the unicast destination IP address to use in outgoing packets when the destination link layer address is not known in the VXLAN device forwarding database, or the multicast IP address to join.

    Format: string

vxlan.rsc
    Specifies whether route short circuit is turned on.

    Format: boolean

vxlan.source-port-max
    Alias: source-port-max

    Specifies the maximum UDP source port to communicate to the remote VXLAN tunnel endpoint.

    Format: uint32

vxlan.source-port-min
    Alias: source-port-min

    Specifies the minimum UDP source port to communicate to the remote VXLAN tunnel endpoint.

    Format: uint32

vxlan.tos
    Specifies the TOS value to use in outgoing packets.

    Format: uint32

vxlan.ttl
    Specifies the time-to-live value to use in outgoing packets.

    Format: uint32

  wifi-p2p setting

Wi-Fi P2P Settings.

Properties:

wifi-p2p.peer
    Alias: peer

    The P2P device that should be connected to. Currently, this is the only way to create or join a group.

    Format: string

wifi-p2p.wfd-ies
    The Wi-Fi Display (WFD) Information Elements (IEs) to set.

    Wi-Fi Display requires a protocol specific information element to be set in certain Wi-Fi frames. These can be specified here for the purpose of establishing a connection. This setting is only useful when implementing a Wi-Fi Display client.

    Format: byte array

wifi-p2p.wps-method
    Flags indicating which mode of WPS is to be used.

    There's little point in changing the default setting as NetworkManager will automatically determine the best method to use.

    Format: uint32

  wimax setting

WiMax Settings.

Properties:

wimax.mac-address
    Alias: mac

    If specified, this connection will only apply to the WiMAX device whose MAC address matches. This property does not change the MAC address of the device (known as MAC spoofing).

    This property is deprecated since version 1.2. WiMAX is no longer supported.

    Format: byte array

wimax.network-name
    Alias: nsp

    Network Service Provider (NSP) name of the WiMAX network this connection should use.

    This property is deprecated since version 1.2. WiMAX is no longer supported.

    Format: string

  802-3-ethernet setting

Alias: ethernet

Wired Ethernet Settings.

Properties:

802-3-ethernet.accept-all-mac-addresses
    When TRUE, setup the interface to accept packets for all MAC addresses. This is enabling the kernel interface flag IFF_PROMISC. When FALSE, the interface will only accept the packets with the interface destination mac address or broadcast.

    Format: NMTernary (int32)

802-3-ethernet.auto-negotiate
    When TRUE, enforce auto-negotiation of speed and duplex mode. If "speed" and "duplex" properties are both specified, only that single mode will be advertised and accepted during the link auto-negotiation process: this works only for BASE-T 802.3 specifications and is useful for enforcing gigabits modes, as in these cases link negotiation is mandatory. When FALSE, "speed" and "duplex" properties should be both set or link configuration will be skipped.

    Format: boolean

802-3-ethernet.cloned-mac-address
    Alias: cloned-mac

    If specified, request that the device use this MAC address instead. This is known as MAC cloning or spoofing.

    Beside explicitly specifying a MAC address, the special values "preserve", "permanent", "random" and "stable" are supported. "preserve" means not to touch the MAC address on activation. "permanent" means to use the permanent hardware address if the device has one (otherwise this is treated as "preserve"). "random" creates a random MAC address on each connect. "stable" creates a hashed MAC address based on connection.stable-id and a machine dependent key.

    If unspecified, the value can be overwritten via global defaults, see manual of NetworkManager.conf. If still unspecified, it defaults to "preserve" (older versions of NetworkManager may use a different default value).

    On D-Bus, this field is expressed as "assigned-mac-address" or the deprecated "cloned-mac-address".

    Format: byte array

802-3-ethernet.duplex
    When a value is set, either "half" or "full", configures the device to use the specified duplex mode. If "auto-negotiate" is "yes" the specified duplex mode will be the only one advertised during link negotiation: this works only for BASE-T 802.3 specifications and is useful for enforcing gigabits modes, as in these cases link negotiation is mandatory. If the value is unset (the default), the link configuration will be either skipped (if "auto-negotiate" is "no", the default) or will be auto-negotiated (if "auto-negotiate" is "yes") and the local device will advertise all the supported duplex modes. Must be set together with the "speed" property if specified. Before specifying a duplex mode be sure your device supports it.

    Format: string

802-3-ethernet.generate-mac-address-mask
    With "cloned-mac-address" setting "random" or "stable", by default all bits of the MAC address are scrambled and a locally-administered, unicast MAC address is created. This property allows to specify that certain bits are fixed. Note that the least significant bit of the first MAC address will always be unset to create a unicast MAC address.

    If the property is NULL, it is eligible to be overwritten by a default connection setting. If the value is still NULL or an empty string, the default is to create a locally-administered, unicast MAC address.

    If the value contains one MAC address, this address is used as mask. The set bits of the mask are to be filled with the current MAC address of the device, while the unset bits are subject to randomization. Setting "FE:FF:FF:00:00:00" means to preserve the OUI of the current MAC address and only randomize the lower 3 bytes using the "random" or "stable" algorithm.

    If the value contains one additional MAC address after the mask, this address is used instead of the current MAC address to fill the bits that shall not be randomized. For example, a value of "FE:FF:FF:00:00:00 68:F7:28:00:00:00" will set the OUI of the MAC address to 68:F7:28, while the lower bits are randomized. A value of "02:00:00:00:00:00 00:00:00:00:00:00" will create a fully scrambled globally-administered, burned-in MAC address.

    If the value contains more than one additional MAC addresses, one of them is chosen randomly. For example, "02:00:00:00:00:00 00:00:00:00:00:00 02:00:00:00:00:00" will create a fully scrambled MAC address, randomly locally or globally administered.

    Format: string

802-3-ethernet.mac-address
    Alias: mac

    If specified, this connection will only apply to the Ethernet device whose permanent MAC address matches. This property does not change the MAC address of the device (i.e. MAC spoofing).

    Format: byte array

802-3-ethernet.mac-address-blacklist
    If specified, this connection will never apply to the Ethernet device whose permanent MAC address matches an address in the list. Each MAC address is in the standard hex-digits-and-colons notation (00:11:22:33:44:55).

    Format: array of string

802-3-ethernet.mtu
    Alias: mtu

    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple Ethernet frames.

    Format: uint32

802-3-ethernet.port
    Specific port type to use if the device supports multiple attachment methods. One of "tp" (Twisted Pair), "aui" (Attachment Unit Interface), "bnc" (Thin Ethernet) or "mii" (Media Independent Interface). If the device supports only one port type, this setting is ignored.

    Format: string

802-3-ethernet.s390-nettype
    s390 network device type; one of "qeth", "lcs", or "ctc", representing the different types of virtual network devices available on s390 systems.

    Format: string

802-3-ethernet.s390-options
    Dictionary of key/value pairs of s390-specific device options. Both keys and values must be strings. Allowed keys include "portno", "layer2", "portname", "protocol", among others. Key names must contain only alphanumeric characters (ie, [a-zA-Z0-9]).

    Currently, NetworkManager itself does nothing with this information. However, s390utils ships a udev rule which parses this information and applies it to the interface.

    Format: dict of string to string

802-3-ethernet.s390-subchannels
    Identifies specific subchannels that this network device uses for communication with z/VM or s390 host. Like the "mac-address" property for non-z/VM devices, this property can be used to ensure this connection only applies to the network device that uses these subchannels. The list should contain exactly 3 strings, and each string may only be composed of hexadecimal characters and the period (.) character.

    Format: array of string

802-3-ethernet.speed
    When a value greater than 0 is set, configures the device to use the specified speed. If "auto-negotiate" is "yes" the specified speed will be the only one advertised during link negotiation: this works only for BASE-T 802.3 specifications and is useful for enforcing gigabit speeds, as in this case link negotiation is mandatory. If the value is unset (0, the default), the link configuration will be either skipped (if "auto-negotiate" is "no", the default) or will be auto-negotiated (if "auto-negotiate" is "yes") and the local device will advertise all the supported speeds. In Mbit/s, ie 100 == 100Mbit/s. Must be set together with the "duplex" property when non-zero. Before specifying a speed value be sure your device supports it.

    Format: uint32

802-3-ethernet.wake-on-lan
    The NMSettingWiredWakeOnLan options to enable. Not all devices support all options. May be any combination of NM_SETTING_WIRED_WAKE_ON_LAN_PHY (0x2), NM_SETTING_WIRED_WAKE_ON_LAN_UNICAST (0x4), NM_SETTING_WIRED_WAKE_ON_LAN_MULTICAST (0x8), NM_SETTING_WIRED_WAKE_ON_LAN_BROADCAST (0x10), NM_SETTING_WIRED_WAKE_ON_LAN_ARP (0x20), NM_SETTING_WIRED_WAKE_ON_LAN_MAGIC (0x40) or the special values NM_SETTING_WIRED_WAKE_ON_LAN_DEFAULT (0x1) (to use global settings) and NM_SETTING_WIRED_WAKE_ON_LAN_IGNORE (0x8000) (to disable management of Wake-on-LAN in NetworkManager).

    Format: uint32

802-3-ethernet.wake-on-lan-password
    If specified, the password used with magic-packet-based Wake-on-LAN, represented as an Ethernet MAC address. If NULL, no password will be required.

    Format: string

  wireguard setting

WireGuard Settings.

Properties:

wireguard.fwmark
    The use of fwmark is optional and is by default off. Setting it to 0 disables it. Otherwise, it is a 32-bit fwmark for outgoing packets.

    Note that "ip4-auto-default-route" or "ip6-auto-default-route" enabled, implies to automatically choose a fwmark.

    Format: uint32

wireguard.ip4-auto-default-route
    Whether to enable special handling of the IPv4 default route. If enabled, the IPv4 default route from wireguard.peer-routes will be placed to a dedicated routing-table and two policy routing rules will be added. The fwmark number is also used as routing-table for the default-route, and if fwmark is zero, an unused fwmark/table is chosen automatically. This corresponds to what wg-quick does with Table=auto and what WireGuard calls "Improved Rule-based Routing".

    Note that for this automatism to work, you usually don't want to set ipv4.gateway, because that will result in a conflicting default route.

    Leaving this at the default will enable this option automatically if ipv4.never-default is not set and there are any peers that use a default-route as allowed-ips. Since this automatism only makes sense if you also have a peer with an /0 allowed-ips, it is usually not necessary to enable this explicitly. However, you can disable it if you want to configure your own routing and rules.

    Format: NMTernary (int32)

wireguard.ip6-auto-default-route
    Like ip4-auto-default-route, but for the IPv6 default route.

    Format: NMTernary (int32)

wireguard.listen-port
    The listen-port. If listen-port is not specified, the port will be chosen randomly when the interface comes up.

    Format: uint32

wireguard.mtu
    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple fragments.

    If zero a default MTU is used. Note that contrary to wg-quick's MTU setting, this does not take into account the current routes at the time of activation.

    Format: uint32

wireguard.peer-routes
    Whether to automatically add routes for the AllowedIPs ranges of the peers. If TRUE (the default), NetworkManager will automatically add routes in the routing tables according to ipv4.route-table and ipv6.route-table. Usually you want this automatism enabled. If FALSE, no such routes are added automatically. In this case, the user may want to configure static routes in ipv4.routes and ipv6.routes, respectively.

    Note that if the peer's AllowedIPs is "0.0.0.0/0" or "::/0" and the profile's ipv4.never-default or ipv6.never-default setting is enabled, the peer route for this peer won't be added automatically.

    Format: boolean

wireguard.private-key
    The 256 bit private-key in base64 encoding.

    Format: string

wireguard.private-key-flags
    Flags indicating how to handle the "private-key" property.

    Format: NMSettingSecretFlags (uint32)

  802-11-wireless setting

Alias: wifi

Wi-Fi Settings.

Properties:

802-11-wireless.ap-isolation
    Configures AP isolation, which prevents communication between wireless devices connected to this AP. This property can be set to a value different from NM_TERNARY_DEFAULT (-1) only when the interface is configured in AP mode.

    If set to NM_TERNARY_TRUE (1), devices are not able to communicate with each other. This increases security because it protects devices against attacks from other clients in the network. At the same time, it prevents devices to access resources on the same wireless networks as file shares, printers, etc.

    If set to NM_TERNARY_FALSE (0), devices can talk to each other.

    When set to NM_TERNARY_DEFAULT (-1), the global default is used; in case the global default is unspecified it is assumed to be NM_TERNARY_FALSE (0).

    Format: NMTernary (int32)

802-11-wireless.band
    802.11 frequency band of the network. One of "a" for 5GHz 802.11a or "bg" for 2.4GHz 802.11. This will lock associations to the Wi-Fi network to the specific band, i.e. if "a" is specified, the device will not associate with the same network in the 2.4GHz band even if the network's settings are compatible. This setting depends on specific driver capability and may not work with all drivers.

    Format: string

802-11-wireless.bssid
    If specified, directs the device to only associate with the given access point. This capability is highly driver dependent and not supported by all devices. Note: this property does not control the BSSID used when creating an Ad-Hoc network and is unlikely to in the future.

    Locking a client profile to a certain BSSID will prevent roaming and also disable background scanning. That can be useful, if there is only one access point for the SSID.

    Format: byte array

802-11-wireless.channel
    Wireless channel to use for the Wi-Fi connection. The device will only join (or create for Ad-Hoc networks) a Wi-Fi network on the specified channel. Because channel numbers overlap between bands, this property also requires the "band" property to be set.

    Format: uint32

802-11-wireless.cloned-mac-address
    Alias: cloned-mac

    If specified, request that the device use this MAC address instead. This is known as MAC cloning or spoofing.

    Beside explicitly specifying a MAC address, the special values "preserve", "permanent", "random" and "stable" are supported. "preserve" means not to touch the MAC address on activation. "permanent" means to use the permanent hardware address of the device. "random" creates a random MAC address on each connect. "stable" creates a hashed MAC address based on connection.stable-id and a machine dependent key.

    If unspecified, the value can be overwritten via global defaults, see manual of NetworkManager.conf. If still unspecified, it defaults to "preserve" (older versions of NetworkManager may use a different default value).

    On D-Bus, this field is expressed as "assigned-mac-address" or the deprecated "cloned-mac-address".

    Format: byte array

802-11-wireless.generate-mac-address-mask
    With "cloned-mac-address" setting "random" or "stable", by default all bits of the MAC address are scrambled and a locally-administered, unicast MAC address is created. This property allows to specify that certain bits are fixed. Note that the least significant bit of the first MAC address will always be unset to create a unicast MAC address.

    If the property is NULL, it is eligible to be overwritten by a default connection setting. If the value is still NULL or an empty string, the default is to create a locally-administered, unicast MAC address.

    If the value contains one MAC address, this address is used as mask. The set bits of the mask are to be filled with the current MAC address of the device, while the unset bits are subject to randomization. Setting "FE:FF:FF:00:00:00" means to preserve the OUI of the current MAC address and only randomize the lower 3 bytes using the "random" or "stable" algorithm.

    If the value contains one additional MAC address after the mask, this address is used instead of the current MAC address to fill the bits that shall not be randomized. For example, a value of "FE:FF:FF:00:00:00 68:F7:28:00:00:00" will set the OUI of the MAC address to 68:F7:28, while the lower bits are randomized. A value of "02:00:00:00:00:00 00:00:00:00:00:00" will create a fully scrambled globally-administered, burned-in MAC address.

    If the value contains more than one additional MAC addresses, one of them is chosen randomly. For example, "02:00:00:00:00:00 00:00:00:00:00:00 02:00:00:00:00:00" will create a fully scrambled MAC address, randomly locally or globally administered.

    Format: string

802-11-wireless.hidden
    If TRUE, indicates that the network is a non-broadcasting network that hides its SSID. This works both in infrastructure and AP mode.

    In infrastructure mode, various workarounds are used for a more reliable discovery of hidden networks, such as probe-scanning the SSID. However, these workarounds expose inherent insecurities with hidden SSID networks, and thus hidden SSID networks should be used with caution.

    In AP mode, the created network does not broadcast its SSID.

    Note that marking the network as hidden may be a privacy issue for you (in infrastructure mode) or client stations (in AP mode), as the explicit probe-scans are distinctly recognizable on the air.

    Format: boolean

802-11-wireless.mac-address
    Alias: mac

    If specified, this connection will only apply to the Wi-Fi device whose permanent MAC address matches. This property does not change the MAC address of the device (i.e. MAC spoofing).

    Format: byte array

802-11-wireless.mac-address-blacklist
    A list of permanent MAC addresses of Wi-Fi devices to which this connection should never apply. Each MAC address should be given in the standard hex-digits-and-colons notation (eg "00:11:22:33:44:55").

    Format: array of string

802-11-wireless.mac-address-randomization
    One of NM_SETTING_MAC_RANDOMIZATION_DEFAULT (0) (never randomize unless the user has set a global default to randomize and the supplicant supports randomization), NM_SETTING_MAC_RANDOMIZATION_NEVER (1) (never randomize the MAC address), or NM_SETTING_MAC_RANDOMIZATION_ALWAYS (2) (always randomize the MAC address).

    This property is deprecated since version 1.4. Use the "cloned-mac-address" property instead.

    Format: uint32

802-11-wireless.mode
    Alias: mode

    Wi-Fi network mode; one of "infrastructure", "mesh", "adhoc" or "ap". If blank, infrastructure is assumed.

    Format: string

802-11-wireless.mtu
    Alias: mtu

    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple Ethernet frames.

    Format: uint32

802-11-wireless.powersave
    One of NM_SETTING_WIRELESS_POWERSAVE_DISABLE (2) (disable Wi-Fi power saving), NM_SETTING_WIRELESS_POWERSAVE_ENABLE (3) (enable Wi-Fi power saving), NM_SETTING_WIRELESS_POWERSAVE_IGNORE (1) (don't touch currently configure setting) or NM_SETTING_WIRELESS_POWERSAVE_DEFAULT (0) (use the globally configured value). All other values are reserved.

    Format: uint32

802-11-wireless.seen-bssids
    A list of BSSIDs (each BSSID formatted as a MAC address like "00:11:22:33:44:55") that have been detected as part of the Wi-Fi network. NetworkManager internally tracks previously seen BSSIDs. The property is only meant for reading and reflects the BSSID list of NetworkManager. The changes you make to this property will not be preserved.

    This is not a regular property that the user would configure. Instead, NetworkManager automatically sets the seen BSSIDs and tracks them internally in "/var/lib/NetworkManager/seen-bssids" file.

    Format: array of string

802-11-wireless.ssid
    Alias: ssid

    SSID of the Wi-Fi network. Must be specified.

    Format: byte array

802-11-wireless.wake-on-wlan
    The NMSettingWirelessWakeOnWLan options to enable. Not all devices support all options. May be any combination of NM_SETTING_WIRELESS_WAKE_ON_WLAN_ANY (0x2), NM_SETTING_WIRELESS_WAKE_ON_WLAN_DISCONNECT (0x4), NM_SETTING_WIRELESS_WAKE_ON_WLAN_MAGIC (0x8), NM_SETTING_WIRELESS_WAKE_ON_WLAN_GTK_REKEY_FAILURE (0x10), NM_SETTING_WIRELESS_WAKE_ON_WLAN_EAP_IDENTITY_REQUEST (0x20), NM_SETTING_WIRELESS_WAKE_ON_WLAN_4WAY_HANDSHAKE (0x40), NM_SETTING_WIRELESS_WAKE_ON_WLAN_RFKILL_RELEASE (0x80), NM_SETTING_WIRELESS_WAKE_ON_WLAN_TCP (0x100) or the special values NM_SETTING_WIRELESS_WAKE_ON_WLAN_DEFAULT (0x1) (to use global settings) and NM_SETTING_WIRELESS_WAKE_ON_WLAN_IGNORE (0x8000) (to disable management of Wake-on-LAN in NetworkManager).

    Format: uint32

  802-11-wireless-security setting

Alias: wifi-sec

Wi-Fi Security Settings.

Properties:

802-11-wireless-security.auth-alg
    When WEP is used (ie, key-mgmt = "none" or "ieee8021x") indicate the 802.11 authentication algorithm required by the AP here. One of "open" for Open System, "shared" for Shared Key, or "leap" for Cisco LEAP. When using Cisco LEAP (ie, key-mgmt = "ieee8021x" and auth-alg = "leap") the "leap-username" and "leap-password" properties must be specified.

    Format: string

802-11-wireless-security.fils
    Indicates whether Fast Initial Link Setup (802.11ai) must be enabled for the connection. One of NM_SETTING_WIRELESS_SECURITY_FILS_DEFAULT (0) (use global default value), NM_SETTING_WIRELESS_SECURITY_FILS_DISABLE (1) (disable FILS), NM_SETTING_WIRELESS_SECURITY_FILS_OPTIONAL (2) (enable FILS if the supplicant and the access point support it) or NM_SETTING_WIRELESS_SECURITY_FILS_REQUIRED (3) (enable FILS and fail if not supported). When set to NM_SETTING_WIRELESS_SECURITY_FILS_DEFAULT (0) and no global default is set, FILS will be optionally enabled.

    Format: int32

802-11-wireless-security.group
    A list of group/broadcast encryption algorithms which prevents connections to Wi-Fi networks that do not utilize one of the algorithms in the list. For maximum compatibility leave this property empty. Each list element may be one of "wep40", "wep104", "tkip", or "ccmp".

    Format: array of string

802-11-wireless-security.key-mgmt
    Key management used for the connection. One of "none" (WEP or no password protection), "ieee8021x" (Dynamic WEP), "owe" (Opportunistic Wireless Encryption), "wpa-psk" (WPA2 + WPA3 personal), "sae" (WPA3 personal only), "wpa-eap" (WPA2 + WPA3 enterprise) or "wpa-eap-suite-b-192" (WPA3 enterprise only).

    This property must be set for any Wi-Fi connection that uses security.

    Format: string

802-11-wireless-security.leap-password
    The login password for legacy LEAP connections (ie, key-mgmt = "ieee8021x" and auth-alg = "leap").

    Format: string

802-11-wireless-security.leap-password-flags
    Flags indicating how to handle the "leap-password" property.

    Format: NMSettingSecretFlags (uint32)

802-11-wireless-security.leap-username
    The login username for legacy LEAP connections (ie, key-mgmt = "ieee8021x" and auth-alg = "leap").

    Format: string

802-11-wireless-security.pairwise
    A list of pairwise encryption algorithms which prevents connections to Wi-Fi networks that do not utilize one of the algorithms in the list. For maximum compatibility leave this property empty. Each list element may be one of "tkip" or "ccmp".

    Format: array of string

802-11-wireless-security.pmf
    Indicates whether Protected Management Frames (802.11w) must be enabled for the connection. One of NM_SETTING_WIRELESS_SECURITY_PMF_DEFAULT (0) (use global default value), NM_SETTING_WIRELESS_SECURITY_PMF_DISABLE (1) (disable PMF), NM_SETTING_WIRELESS_SECURITY_PMF_OPTIONAL (2) (enable PMF if the supplicant and the access point support it) or NM_SETTING_WIRELESS_SECURITY_PMF_REQUIRED (3) (enable PMF and fail if not supported). When set to NM_SETTING_WIRELESS_SECURITY_PMF_DEFAULT (0) and no global default is set, PMF will be optionally enabled.

    Format: int32

802-11-wireless-security.proto
    List of strings specifying the allowed WPA protocol versions to use. Each element may be one "wpa" (allow WPA) or "rsn" (allow WPA2/RSN). If not specified, both WPA and RSN connections are allowed.

    Format: array of string

802-11-wireless-security.psk
    Pre-Shared-Key for WPA networks. For WPA-PSK, it's either an ASCII passphrase of 8 to 63 characters that is (as specified in the 802.11i standard) hashed to derive the actual key, or the key in form of 64 hexadecimal character. The WPA3-Personal networks use a passphrase of any length for SAE authentication.

    Format: string

802-11-wireless-security.psk-flags
    Flags indicating how to handle the "psk" property.

    Format: NMSettingSecretFlags (uint32)

802-11-wireless-security.wep-key-flags
    Flags indicating how to handle the "wep-key0", "wep-key1", "wep-key2", and "wep-key3" properties.

    Format: NMSettingSecretFlags (uint32)

802-11-wireless-security.wep-key-type
    Controls the interpretation of WEP keys. Allowed values are NM_WEP_KEY_TYPE_KEY (1), in which case the key is either a 10- or 26-character hexadecimal string, or a 5- or 13-character ASCII password; or NM_WEP_KEY_TYPE_PASSPHRASE (2), in which case the passphrase is provided as a string and will be hashed using the de-facto MD5 method to derive the actual WEP key.

    Format: NMWepKeyType (uint32)

802-11-wireless-security.wep-key0
    Index 0 WEP key. This is the WEP key used in most networks. See the "wep-key-type" property for a description of how this key is interpreted.

    Format: string

802-11-wireless-security.wep-key1
    Index 1 WEP key. This WEP index is not used by most networks. See the "wep-key-type" property for a description of how this key is interpreted.

    Format: string

802-11-wireless-security.wep-key2
    Index 2 WEP key. This WEP index is not used by most networks. See the "wep-key-type" property for a description of how this key is interpreted.

    Format: string

802-11-wireless-security.wep-key3
    Index 3 WEP key. This WEP index is not used by most networks. See the "wep-key-type" property for a description of how this key is interpreted.

    Format: string

802-11-wireless-security.wep-tx-keyidx
    When static WEP is used (ie, key-mgmt = "none") and a non-default WEP key index is used by the AP, put that WEP key index here. Valid values are 0 (default key) through 3. Note that some consumer access points (like the Linksys WRT54G) number the keys 1 - 4.

    Format: uint32

802-11-wireless-security.wps-method
    Flags indicating which mode of WPS is to be used if any.

    There's little point in changing the default setting as NetworkManager will automatically determine whether it's feasible to start WPS enrollment from the Access Point capabilities.

    WPS can be disabled by setting this property to a value of 1.

    Format: uint32

  wpan setting

IEEE 802.15.4 (WPAN) MAC Settings.

Properties:

wpan.channel
    Alias: channel

    IEEE 802.15.4 channel. A positive integer or -1, meaning "do not set, use whatever the device is already set to".

    Format: int32

wpan.mac-address
    Alias: mac

    If specified, this connection will only apply to the IEEE 802.15.4 (WPAN) MAC layer device whose permanent MAC address matches.

    Format: string

wpan.page
    Alias: page

    IEEE 802.15.4 channel page. A positive integer or -1, meaning "do not set, use whatever the device is already set to".

    Format: int32

wpan.pan-id
    Alias: pan-id

    IEEE 802.15.4 Personal Area Network (PAN) identifier.

    Format: uint32

wpan.short-address
    Alias: short-addr

    Short IEEE 802.15.4 address to be used within a restricted environment.

    Format: uint32

  bond-port setting

Bond Port Settings.

Properties:

bond-port.prio
    Alias: prio

    The port priority for bond active port re-selection during failover. A higher number means a higher priority in selection. The primary port has the highest priority. This option is only compatible with active-backup, balance-tlb and balance-alb modes.

    Format: int32

bond-port.queue-id
    Alias: queue-id

    The queue ID of this bond port. The maximum value of queue ID is the number of TX queues currently active in device.

    Format: uint32

  hostname setting

Hostname settings.

Properties:

hostname.from-dhcp
    Whether the system hostname can be determined from DHCP on this connection.

    When set to NM_TERNARY_DEFAULT (-1), the value from global configuration is used. If the property doesn't have a value in the global configuration, NetworkManager assumes the value to be NM_TERNARY_TRUE (1).

    Format: NMTernary (int32)

hostname.from-dns-lookup
    Whether the system hostname can be determined from reverse DNS lookup of addresses on this device.

    When set to NM_TERNARY_DEFAULT (-1), the value from global configuration is used. If the property doesn't have a value in the global configuration, NetworkManager assumes the value to be NM_TERNARY_TRUE (1).

    Format: NMTernary (int32)

hostname.only-from-default
    If set to NM_TERNARY_TRUE (1), NetworkManager attempts to get the hostname via DHCPv4/DHCPv6 or reverse DNS lookup on this device only when the device has the default route for the given address family (IPv4/IPv6).

    If set to NM_TERNARY_FALSE (0), the hostname can be set from this device even if it doesn't have the default route.

    When set to NM_TERNARY_DEFAULT (-1), the value from global configuration is used. If the property doesn't have a value in the global configuration, NetworkManager assumes the value to be NM_TERNARY_FALSE (0).

    Format: NMTernary (int32)

hostname.priority
    The relative priority of this connection to determine the system hostname. A lower numerical value is better (higher priority). A connection with higher priority is considered before connections with lower priority.

    If the value is zero, it can be overridden by a global value from NetworkManager configuration. If the property doesn't have a value in the global configuration, the value is assumed to be 100.

    Negative values have the special effect of excluding other connections with a greater numerical priority value; so in presence of at least one negative priority, only connections with the lowest priority value will be used to determine the hostname.

    Format: int32

  link setting

Link settings.

Properties:

link.gro-max-size
    The maximum size of a packet built by the Generic Receive Offload stack for this device. The value must be between 0 and 4294967295. When set to -1, the existing value is preserved.

    Format: int64

link.gso-max-segments
    The maximum segments of a Generic Segment Offload packet the device should accept. The value must be between 0 and 4294967295. When set to -1, the existing value is preserved.

    Format: int64

link.gso-max-size
    The maximum size of a Generic Segment Offload packet the device should accept. The value must be between 0 and 4294967295. When set to -1, the existing value is preserved.

    Format: int64

link.tx-queue-length
    The size of the transmit queue for the device, in number of packets. The value must be between 0 and 4294967295. When set to -1, the existing value is preserved.

    Format: int64

  loopback setting

Loopback Link Settings.

Properties:

loopback.mtu
    Alias: mtu

    If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple Ethernet frames.

    Format: uint32

  veth setting

Veth Settings.

Properties:

veth.peer
    Alias: peer

    This property specifies the peer interface name of the veth. This property is mandatory.

    Format: string

  Secret flag types:

Each password or secret property in a setting has an associated flags property that describes how to handle that secret. The flags property is a bitfield that contains zero or more of the following values logically OR-ed together.

    • 0x0 (none) - the system is responsible for providing and storing this secret. This may be required so that secrets are already available before the user logs in. It also commonly means that the secret will be stored in plain text on disk, accessible to root only. For example via the keyfile settings plugin as described in the "PLUGINS" section in NetworkManager.conf(5).

    • 0x1 (agent-owned) - a user-session secret agent is responsible for providing and storing this secret; when it is required, agents will be asked to provide it.

    • 0x2 (not-saved) - this secret should not be saved but should be requested from the user each time it is required. This flag should be used for One-Time-Pad secrets, PIN codes from hardware tokens, or if the user simply does not want to save the secret.

    • 0x4 (not-required) - in some situations it cannot be automatically determined that a secret is required or not. This flag hints that the secret is not required and should not be requested from the user.

FILES

/etc/NetworkManager/system-connections or distro plugin-specific location

SEE ALSO

nmcli(1), nmcli-examples(7), NetworkManager(8), nm-settings-dbus(5), nm-settings-keyfile(5), NetworkManager.conf(5)