BRIDGE(8)

NAME
bridge - show / manipulate bridge addresses and devices

SYNOPSIS
bridge [ OPTIONS ] OBJECT { COMMAND | help }

OBJECT := { link | fdb | mdb | vlan | monitor }

OPTIONS := { -V[ersion] | -s[tatistics] | -n[etns] name | -b[atch] filename | -c[lor] | -p[retty] | -j[son] | -o[neline] }
bridge link set dev DEV [ cost COST ] [ priority PRIO ] [ state STATE ] [ guard { on | off } ] [ hairpin { on | off } ] [ fastleave { on | off } ] [ root_block { on | off } ] [ learning { on | off } ] [ learning_sync { on | off } ] [ flood { on | off } ] [ hwmode { vepa | veb } ] [ mcast_flood { on | off } ] [ neigh_suppress { on | off } ] [ vlan_tunnel { on | off } ] [ isolated { on | off } ] [ backup_port DEVICE ] [ nobackup_port ] [ self ] [ master ]
bridge link [ show ] [ dev DEV ]
bridge fdb { add | append | del | replace } LLADDR dev DEV { local | static | dynamic } [ self ] [ master ] [ router ] [ use ] [ extern_learn ] [ sticky ] [ dst IPADDR ] [ vni VNI ] [ port PORT ] [ via DEVICE ]
bridge fdb [ show ] [ dev DEV ] [ br BRDEV ] [ brport DEV ] [ vlan VID ] [ state STATE ]
bridge mdb { add | del } dev DEV port PORT grp GROUP [ permanent | temp ] [ vid VID ]
bridge mdb show [ dev DEV ]
bridge vlan { add | del } dev DEV vid VID [ tunnel_info TUNNEL_ID ] [ pvid ] [ untagged ] [ self ] [ master ]
bridge vlan [ show | tunnelshow ] [ dev DEV ]
bridge monitor [ all | neigh | link | mdb ]

OPTIONS

-V, -Version
    print the version of the bridge utility and exit.

-s, -stats, -statistics
    output more information. If this option is given multiple times, the amount of information increases. As a rule, the information is statistics or some time values.

-d, -details
    print detailed information about MDB router ports.

-n, -net, -netns <NETNS>
    switches bridge to the specified network namespace NETNS. Actually it just simplifies executing of: ip netns exec NETNS bridge [ OPTIONS ] OBJECT { COMMAND | help } to bridge -n[etns] NETNS [ OPTIONS ] OBJECT { COMMAND | help }

-b, -batch <FILENAME>
    Read commands from provided file or standard input and invoke them. First failure will cause termination of bridge command.

-force
    Don't terminate bridge command on errors in batch mode. If there were any errors during execution of the commands, the application return code will be non zero.

-c[color][={always|auto|never}
    Configure color output. If parameter is omitted or always, color output is enabled regardless of stdout state. If parameter is auto, stdout is checked to be a terminal before enabling color output. If parameter is never, color output is disabled. If specified multiple times, the last one takes precedence. This flag is ignored if -json is also given.

-j, -json
    Output results in JavaScript Object Notation (JSON).

-p, -pretty
    When combined with -j generate a pretty JSON output.

-o, -oneline
    output each record on a single line, replacing line feeds with the '\' character. This is convenient when you want to count records with wc(1) or to grep(1) the output.

BRIDGE - COMMAND SYNTAX

  OBJECT

link
    - Bridge port.

fdb - Forwarding Database entry.

mdb - Multicast group database entry.

vlan
    - VLAN filter list.

  COMMAND
Specifies the action to perform on the object. The set of possible actions depends on the object type. As a rule, it is possible to add, delete and show (or list ) objects, but some objects do not allow all of these operations or have some additional commands. The help command is available for all objects. It prints out a list of available commands and argument syntax conventions.

If no command is given, some default command is assumed. Usually it is list or, if the objects of this class cannot be listed, help.

bridge link - bridge port
link objects correspond to the port devices of the bridge.

The corresponding commands set and display port status and bridge specific attributes.

  bridge link set - set bridge specific attributes on a port

dev NAME
    interface name of the bridge port

cost COST
    the STP path cost of the specified port.

priority PRIO
    the STP port priority. The priority value is an unsigned 8-bit quantity (number between 0 and 255). This metric is used in the designated port an droot port selectio algorithms.

state STATE
    the operation state of the port. This is primarily used by user space STP/RSTP implementation. One may enter a lowercased port state name, or one of the numbers below. Negative inputs are ignored, and unrecognized names return an error. 0 - port is DISABLED. Make this port completely inactive.

    1 - STP LISTENING state. Only valid if STP is enabled on the bridge. In this state the port listens for STP BPDUs and drops all other traffic frames.

    2 - STP LEARNING state. Only valid if STP is enabled on the bridge. In this state the port will accept traffic only for the purpose of updating MAC address tables.

    3 - STP FORWARDING state. Port is fully active.

    4 - STP BLOCKING state. Only valid if STP is enabled on the bridge. This state is used during the STP election process. In this state, port will only process STP BPDUs.

guard on or guard off
    Controls whether STP BPDUs will be processed by the bridge port. By default, the flag is turned off allowed BPDU processing. Turning this flag on will cause the port to stop processing STP BPDUs.

hairpin on or hairpin off
    Controls whether traffic may be send back out of the port on which it was received. By default, this flag is turned off and the bridge will not forward traffic back out of the receiving port.

fastleave on or fastleave off
    This flag allows the bridge to immediately stop multicast traffic on a port that receives IGMP Leave message. It is only used with IGMP snooping is enabled on the bridge. By default the flag is off.

root_block on or root_block off
    Controls whether a given port is allowed to become root port or not. Only used when STP is enabled on the bridge. By default the flag is off.

learning on or learning off
    Controls whether a given port will learn MAC addresses from received traffic or not. If learning if off, the bridge will end up flooding any traffic for which it has no FDB entry. By default this flag is on.

learning_sync on or learning_sync off
    Controls whether a given port will sync MAC addresses learned on device port to bridge FDB.

flooding on or flooding off
    Controls whether a given port will flood unicast traffic for which there is no FDB entry. By default this flag is on.

hwmode
    Some network interface cards support HW bridge functionality and they may be configured in different modes. Currently support modes are: vepa - Data sent between HW ports is sent on the wire to the external switch. veb - bridging happens in hardware.

mcast_flood on or mcast_flood off
    Controls whether a given port will be flooded with multicast traffic for which there is no MDB entry. By default this flag is on.

neigh_suppress on or neigh_suppress off
    Controls whether neigh discovery (arp and nd) proxy and suppression is enabled on the port. By default this flag is off.

vlan_tunnel on or vlan_tunnel off
    Controls whether vlan to tunnel mapping is enabled on the port. By default this flag is off.

isolated on or isolated off
    Controls whether a given port will be isolated, which means it will be able to communicate with non-isolated ports only. By default this flag is off.

backup_port DEVICE
    If the port loses carrier all traffic will be redirected to the configured backup port

nobackup_port
    Removes the currently configured backup port

self
    link setting is configured on specified physical device

master
    link setting is configured on the software bridge (default)

-t, -timestamp
    display current time when using monitor option.

  bridge link show - list bridge port configuration.
This command displays the current bridge port configuration and flags.

bridge fdb - forwarding database management
fdb objects contain known Ethernet addresses on a link.

The corresponding commands display fdb entries, add new entries, append entries, and delete old ones.

  bridge fdb add - add a new fdb entry
This command creates a new fdb entry.

LLADDR
    the Ethernet MAC address.

dev DEV
    the interface to which this address is associated. local - is a local permanent fdb entry

    static - is a static (no arp) fdb entry

    dynamic - is a dynamic reachable age-able fdb entry

    self - the address is associated with the port drivers fdb. Usually hardware.

    master - the address is associated with master devices fdb. Usually software (default).

    router - the destination address is associated with a router. Valid if the referenced device is a VXLAN type device and has route shortcircuit enabled.

    use - the address is in use. User space can use this option to indicate to the kernel that the fdb entry is in use.

    extern_learn - this entry was learned externally. This option can be used to indicate to the kernel that an entry was hardware or user-space controller learnt dynamic entry. Kernel will not age such an entry.

    sticky - this entry will not change its port due to learning.

    The next command line parameters apply only when the specified device DEV is of type VXLAN.

dst IPADDR
    the IP address of the destination VXLAN tunnel endpoint where the Ethernet MAC ADDRESS resides.

vni VNI
    the VXLAN VNI Network Identifier (or VXLAN Segment ID) to use to connect to the remote VXLAN tunnel endpoint. If omitted the value specified at vxlan device creation will be used.

port PORT
    the UDP destination PORT number to use to connect to the remote VXLAN tunnel endpoint. If omitted the default value is used.

via DEVICE
    device name of the outgoing interface for the VXLAN device driver to reach the remote VXLAN tunnel endpoint.

  bridge fdb append - append a forwarding database entry
This command adds a new fdb entry with an already known LLADDR. Valid only for multicast link layer addresses. The command adds support for broadcast and multicast Ethernet MAC addresses. The Ethernet MAC address is added multiple times into the forwarding database and the vxlan device driver sends a copy of the data packet to each entry found.

The arguments are the same as with bridge fdb add.

  bridge fdb delete - delete a forwarding database entry
This command removes an existing fdb entry.

The arguments are the same as with bridge fdb add.

  bridge fdb replace - replace a forwarding database entry
If no matching entry is found, a new one will be created instead.

The arguments are the same as with bridge fdb add.

  bridge fdb show - list forwarding entries.
This command displays the current forwarding table.

With the -statistics option, the command becomes verbose. It prints out the last updated and last used time for each entry.

bridge mdb - multicast group database management
mdb objects contain known IP multicast group addresses on a link.

The corresponding commands display mdb entries, add new entries, and delete old ones.

  bridge mdb add - add a new multicast group database entry
This command creates a new mdb entry.

dev DEV
    the interface where this group address is associated.

port PORT
    the port whose link is known to have members of this multicast group.

grp GROUP
    the IP multicast group address whose members reside on the link connected to the port. permanent - the mdb entry is permanent

    temp - the mdb entry is temporary (default)

vid VID
    the VLAN ID which is known to have members of this multicast group.

  bridge mdb delete - delete a multicast group database entry
This command removes an existing mdb entry.

The arguments are the same as with bridge mdb add.

  bridge mdb show - list multicast group database entries
This command displays the current multicast group membership table. The table is populated by IGMP and MLD snooping in the bridge driver automatically. It can be altered by bridge mdb add and bridge mdb del commands manually too.

dev DEV
    the interface only whose entries should be listed. Default is to list all bridge interfaces.

With the -details option, the command becomes verbose. It prints out the ports known to have a connected router.

With the -statistics option, the command displays timer values for mdb and router port entries.

bridge vlan - VLAN filter list
vlan objects contain known VLAN IDs for a link.

The corresponding commands display vlan filter entries, add new entries, and delete old ones.

  bridge vlan add - add a new vlan filter entry
This command creates a new vlan filter entry.

dev NAME
    the interface with which this vlan is associated.

vid VID
    the VLAN ID that identifies the vlan.

tunnel_info TUNNEL_ID
    the TUNNEL ID that maps to this vlan. The tunnel id is set in dst_metadata for every packet that belongs to this vlan (applicable to bridge ports with vlan_tunnel flag set).

pvid
    the vlan specified is to be considered a PVID at ingress. Any untagged frames will be assigned to this VLAN.

untagged
    the vlan specified is to be treated as untagged on egress.

self
    the vlan is configured on the specified physical device. Required if the device is the bridge device.

master
    the vlan is configured on the software bridge (default).

  bridge vlan delete - delete a vlan filter entry
This command removes an existing vlan filter entry.

The arguments are the same as with bridge vlan add. The pvid and untagged flags are ignored.

  bridge vlan show - list vlan configuration.
This command displays the current VLAN filter table.

With the -statistics option, the command displays per-vlan traffic statistics.

  bridge vlan tunnelshow - list vlan tunnel mapping.
This command displays the current vlan tunnel info mapping.

bridge monitor - state monitoring
The bridge utility can monitor the state of devices and addresses continuously. This option has a slightly different format. Namely, the monitor command is the first in the command line and then the object list follows: bridge monitor [ all | OBJECT-LIST ] OBJECT-LIST is the list of object types that we want to monitor. It may contain link, fdb, and mdb. If no file argument is given, bridge opens RTNETLINK, listens on it and dumps state changes in the format described in previous sections.

If a file name is given, it does not listen on RTNETLINK, but opens the file containing RTNETLINK messages saved in binary format and dumps them.

NOTES
This command uses facilities added in Linux 3.0. Although the forwarding table is maintained on a per-bridge device basis the bridge device is not part of the syntax. This is a limitation of the underlying netlink neighbour message protocol. When displaying the forwarding table, entries for all bridges are displayed. Add/delete/modify commands determine the underlying bridge device based on the bridge to which the corresponding ethernet device is attached.

SEE ALSO
ip(8)

BUGS
Please direct bugreports and patches to: <netdev@vger.kernel.org>

AUTHOR
Original Manpage by Stephen Hemminger