IP-NEXTHOP(8)

NAME
ip-nexthop - nexthop object management

SYNOPSIS

ip [ ip-OPTIONS ] nexthop { COMMAND | help }

ip nexthop { show | flush } SELECTOR
ip nexthop { add | replace } id ID NH
ip nexthop { get | del } id ID
ip nexthop bucket list BUCKET_SELECTOR
ip nexthop bucket get id ID index INDEX
SELECTOR := [ id ID ] [ dev DEV ] [ vrf NAME ] [ master DEV ] [ groups ] [ fdb ]
BUCKET_SELECTOR := SELECTOR | [ nhid ID ]
NH := { blackhole | [ via ADDRESS ] [ dev DEV ] [ onlink ] [ encap ENCAP ] [ fdb ] | group GROUP [ fdb ] [ type TYPE [ TYPE_ARGS ] ] }
ENCAP := [ ENCAP_MPLS ]
ENCAP_MPLS := mpls [ LABEL ] [ ttl TTL ]
GROUP := id[,weight[/...]
TYPE := { mpath | resilient }
TYPE_ARGS := [ RESILIENT_ARGS ]
RESILIENT_ARGS := [ buckets BUCKETS ] [ idle_timer IDLE ] [ unbalanced_timer UNBALANCED ]

DESCRIPTION
ip nexthop is used to manipulate entries in the kernel's nexthop tables.

ip nexthop add id ID
    add new nexthop entry

ip nexthop replace id ID
    change the configuration of a nexthop or add new one

    via [ FAMILY ] ADDRESS
        the address of the nexthop router, in the address family FAMILY. Address family must match address family of nexthop instance.

    dev NAME
        is the output device.

    onlink
        pretend that the nexthop is directly attached to this link, even if it does not match any interface prefix.

    encap ENCAPTYPE ENCAPHDR
        attach tunnel encapsulation attributes to this route.

        ENCAPTYPE is a string specifying the supported encapsulation type. Namely:
        mpls - encapsulation type MPLS

        ENCAPHDR is a set of encapsulation attributes specific to the ENCAPTYPE.
        mpls
        MPLSLABEL - mpls label stack with labels separated by /

        ttl TTL - TTL to use for MPLS header or 0 to inherit from IP header

    group GROUP [ type TYPE [ TYPE_ARGS ] ]
        create a nexthop group. Group specification is id with an optional weight (id,weight) and a '/' as a separator between entries.

        TYPE is a string specifying the nexthop group type. Namely:
        mpath - Multipath nexthop group backed by the hash-threshold algorithm. The default when the type is unspecified.

        resilient - Resilient nexthop group. Group is resilient to addition and deletion of nexthops.

        TYPE_ARGS is a set of attributes specific to the TYPE.
        resilient
        buckets BUCKETS - Number of nexthop buckets. Cannot be changed for an existing group

        idle_timer IDLE - Time in seconds in which a nexthop bucket does not see traffic and is therefore considered idle. Default is 120 seconds unbalanced_timer UNBALANCED - Time in seconds in which a nexthop group is unbalanced and is therefore considered unbalanced. The kernel will try to rebalance unbalanced groups, which might result in some flows being reset. A value of 0 means that no rebalancing will take place. Default is 0 seconds

    blackhole
        create a blackhole nexthop

    fdb nexthop and nexthop groups for use with layer-2 fdb entries. A fdb nexthop group can only have fdb nexthops. Example: Used to represent a vxlan remote vtep ip. layer-2 vxlan fdb entry pointing to an ecmp nexthop group containing multiple remote vtep ips.

ip nexthop delete id ID
    delete nexthop with given id.

ip nexthop show
    show the contents of the nexthop table or the nexthops selected by some criteria.

    dev DEV
        show the nexthops using the given device.

    vrf NAME
        show the nexthops using devices associated with the vrf name

    master DEV
        show the nexthops using devices enslaved to given master device

    groups
        show only nexthop groups

    fdb show only fdb nexthops and nexthop groups

ip nexthop flush
    flushes nexthops selected by some criteria. Criteria options are the same as show.

ip nexthop get id ID
    get a single nexthop by id

ip nexthop bucket show
    show the contents of the nexthop bucket table or the nexthop buckets selected by some criteria.

    id ID
        show the nexthop buckets that belong to a nexthop group with a given id

    nhid ID
        show the nexthop buckets that hold a nexthop with a given id

    dev DEV
        show the nexthop buckets using the given device

    vrf NAME
        show the nexthop buckets using devices associated with the vrf name

    master DEV
        show the nexthop buckets using devices enslaved to given master device

ip nexthop bucket get id ID index INDEX
    get a single nexthop bucket by nexthop group id and bucket index

EXAMPLES

ip nexthop ls
    Show all nexthop entries in the kernel.

ip nexthop add id 1 via 192.168.1.1 dev eth0
    Adds an IPv4 nexthop with id 1 using the gateway 192.168.1.1 out device eth0.

ip nexthop add id 2 encap mpls 200/300 via 10.1.1.1 dev eth0
    Adds an IPv4 nexthop with mpls encapsulation attributes attached to it.

ip nexthop add id 3 group 1/2
    Adds a nexthop with id 3. The nexthop is a group using nexthops with ids 1 and 2 at equal weight.

ip nexthop add id 4 group 1,5/2,11
    Adds a nexthop with id 4. The nexthop is a group using nexthops with ids 1 and 2 with nexthop 1 at weight 5 and nexthop 2 at weight 11.

ip nexthop add id 5 via 192.168.1.2 fdb
    Adds a fdb nexthop with id 5.

ip nexthop add id 7 group 5/6 fdb
    Adds a fdb nexthop group with id 7. A fdb nexthop group can only have fdb nexthops.

ip nexthop add id 10 group 1/2 type resilient buckets 32
    Add a resilient nexthop group with id 10 and 32 nexthop buckets.

SEE ALSO
ip(8)

AUTHOR
Original Manpage by David Ahern <dsahern@kernel.org>