RDMA-DEV(8)

NAME
rdma-dev - RDMA device configuration

SYNOPSIS

rdma [ OPTIONS ] dev { COMMAND | help }

OPTIONS := { -V[ersion] | -d[etails] }
rdma dev show [ DEV ]
rdma dev set [ DEV ] name NEWNAME
rdma dev set [ DEV ] netns NSNAME
rdma dev set [ DEV ] adaptive-moderation [on/off]
rdma dev help

DESCRIPTION

  rdma dev set - rename RDMA device or set network namespace or set RDMA device adaptive-moderation

  rdma dev show - display RDMA device attributes

DEV - specifies the RDMA device to show. If this argument is omitted all devices are listed.

EXAMPLES

rdma dev
    Shows the state of all RDMA devices on the system.

rdma dev show mlx5_3
    Shows the state of specified RDMA device.

rdma dev set mlx5_3 name rdma_0
    Renames the mlx5_3 device to rdma_0.

rdma dev set mlx5_3 netns foo
    Changes the network namespace of RDMA device to foo where foo is previously created using iproute2 ip command.

rdma dev set mlx5_3 adaptive-moderation [on/off]
    Sets the state of adaptive interrupt moderation for the RDMA device.
    This is a global setting for the RDMA device but the value is printed for each CQ individually because the state is constant from CQ allocation.

SEE ALSO
ip(8), rdma(8), rdma-link(8), rdma-resource(8), rdma-system(8), rdma-statistic(8),

AUTHOR
Leon Romanovsky <leonro@mellanox.com>