#playback_rcv
#playback_rcv_hp
enable
TERT_TDM_RX_0 Audio Mixer MultiMedia1:1
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:One
TERT_TDM_RX_0 Format:S24_LE
RCV PCM Source:ASP
RCV AMP PCM Gain:0
RCV DRE DRE Switch:1
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:DSPTX1
RCV DSP RX1 Source:ASPRX1
RCV DSP RX2 Source:ASPRX2
RCV ASPRX1 Slot Position:0:
RCV ASPRX2 Slot Position:2:
disable
TERT_TDM_RX_0 Audio Mixer MultiMedia1:0
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:Two
TERT_TDM_RX_0 Format:S24_LE
RCV PCM Source:None
RCV AMP PCM Gain:0
RCV DRE DRE Switch:1
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:Zero
RCV DSP RX1 Source:Zero
RCV DSP RX2 Source:Zero

#playback_spk
#playback_spk_hp
enable
TERT_TDM_RX_0 Audio Mixer MultiMedia1:1
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:Two
TERT_TDM_RX_0 Format:S24_LE
PCM Source:ASP
RCV PCM Source:ASP
AMP PCM Gain:18
RCV AMP PCM Gain:18
DRE DRE Switch:1
RCV DRE DRE Switch:1
DSP RX1 Source:ASPRX1
DSP RX2 Source:ASPRX1
ASPRX1 Slot Position:1
ASPRX2 Slot Position:4
RCV DSP RX1 Source:ASPRX1
RCV DSP RX2 Source:ASPRX2
RCV ASPRX1 Slot Position:0
RCV ASPRX2 Slot Position:2
ASP TX1 Source:DSPTX1
ASP TX2 Source:Zero
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:DSPTX1

disable
Cirrus SP Usecase Config:Music
PCM Source:None
RCV PCM Source:None
AMP PCM Gain:18
RCV AMP PCM Gain:0
TERT_TDM_RX_0 Audio Mixer MultiMedia1:0
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:Two
TERT_TDM_RX_0 Format:S24_LE
DRE DRE Switch:1
RCV DRE DRE Switch:1
DSP RX1 Source:Zero
DSP RX2 Source:Zero
RCV DSP RX1 Source:Zero
RCV DSP RX2 Source:Zero
ASP TX1 Source:Zero
ASP TX2 Source:Zero
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:Zero

#playback_top-spk
#playback_top-spk_hp
enable
TERT_TDM_RX_0 Audio Mixer MultiMedia1:1
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:One
TERT_TDM_RX_0 Format:S24_LE
PCM Source:None
RCV PCM Source:ASP
RCV AMP PCM Gain:18
RCV DRE DRE Switch:1
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:DSPTX1
RCV DSP RX1 Source:ASPRX1
RCV DSP RX2 Source:ASPRX2
RCV ASPRX1 Slot Position:0
RCV ASPRX2 Slot Position:2


disable
Cirrus SP Usecase Config:Music
PCM Source:None
RCV PCM Source:None
RCV AMP PCM Gain:0
TERT_TDM_RX_0 Audio Mixer MultiMedia1:0
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:Two
TERT_TDM_RX_0 Format:S24_LE
RCV DRE DRE Switch:1
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:Zero
RCV DSP RX1 Source:Zero
RCV DSP RX2 Source:Zero


#playback_bot-spk
#playback_bot-spk_hp
enable
TERT_TDM_RX_0 Audio Mixer MultiMedia1:1
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:Two
TERT_TDM_RX_0 Format:S24_LE
PCM Source:ASP
RCV PCM Source:None
AMP PCM Gain:18
DRE DRE Switch:1
DSP RX1 Source:ASPRX1
DSP RX2 Source:ASPRX1
ASPRX1 Slot Position:1
ASPRX2 Slot Position:4
ASP TX1 Source:DSPTX1
ASP TX2 Source:Zero


disable
Cirrus SP Usecase Config:Music
PCM Source:None
RCV PCM Source:None
AMP PCM Gain:18
TERT_TDM_RX_0 Audio Mixer MultiMedia1:0
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Channels:Two
TERT_TDM_RX_0 Format:S24_LE
DRE DRE Switch:1
DSP RX1 Source:Zero
DSP RX2 Source:Zero
ASP TX1 Source:Zero
ASP TX2 Source:Zero



#playback_headphone
enable
RX_CDC_DMA_RX_0 Audio Mixer MultiMedia1:1
RX_MACRO RX0 MUX:AIF1_PB
RX_MACRO RX1 MUX:AIF1_PB
RX_CDC_DMA_RX_0 Channels:Two
RX INT0_1 MIX1 INP0:RX0
RX INT1_1 MIX1 INP0:RX1
RX INT0 DEM MUX:CLSH_DSM_OUT
RX INT1 DEM MUX:CLSH_DSM_OUT
RX_HPH_PWR_MODE:LOHIFI
RX HPH Mode:CLS_H_LOHIFI
RX_COMP1 Switch:1
RX_COMP2 Switch:1
HPHL_COMP Switch:1
HPHR_COMP Switch:1
HPHL_RDAC Switch:1
HPHR_RDAC Switch:1


disable
RX_CDC_DMA_RX_0 Audio Mixer MultiMedia1:0
RX_MACRO RX0 MUX:ZERO
RX_MACRO RX1 MUX:ZERO
RX_CDC_DMA_RX_0 Channels:One
RX INT0_1 MIX1 INP0:ZERO
RX INT1_1 MIX1 INP0:ZERO
RX INT0 DEM MUX:NORMAL_DSM_OUT
RX INT1 DEM MUX:NORMAL_DSM_OUT
RX_COMP1 Switch:0
RX_COMP2 Switch:0
HPHL_COMP Switch:0
HPHR_COMP Switch:0
HPHL_RDAC Switch:0
HPHR_RDAC Switch:0




#playback_us
enable
TERT_TDM_RX_0 Audio Mixer MultiMedia1:1
TERT_TDM_RX_0 SampleRate:KHZ_96
TERT_TDM_RX_0 Format:S24_LE
TERT_TDM_RX_0 Channels:One
Audio Stream 0 App Type Cfg:69936 10001 96000 87 0
PCM Source:None
RCV PCM Source:DSP
RCV AMP PCM Gain:0
RCV DRE DRE Switch:1
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:DSPTX1
RCV DSP RX1 Source:ASPRX1
RCV DSP RX2 Source:ASPRX2
RCV ASPRX1 Slot Position:0
RCV ASPRX2 Slot Position:2


disable
Cirrus SP Usecase Config:Music
PCM Source:None
RCV PCM Source:None
Audio Stream 0 App Type Cfg:69936 10001 48000 87 0
RCV AMP PCM Gain:0
RCV DRE DRE Switch:1
TERT_TDM_RX_0 Channels:Two
TERT_TDM_RX_0 Audio Mixer MultiMedia1:0
RCV ASP TX1 Source:Zero
RCV ASP TX2 Source:Zero
RCV DSP RX1 Source:Zero
RCV DSP RX2 Source:Zero

#capture_main-mic
#enable_main-mic
enable
TX DEC1 MUX:SWR_MIC
TX SMIC MUX1:SWR_MIC4
TX_AIF1_CAP Mixer DEC1:1
TX0 MODE:ADC_LP
ADC1 ChMap:SWRM_TX2_CH1
TX_CDC_DMA_TX_3 Channels:One
ADC1_MIXER Switch:1
ADC1 Volume:8
MultiMedia1 Mixer TX_CDC_DMA_TX_3:1
TX_CDC_DMA_TX_3 SampleRate:$rate

#disable_main-mic
disable
TX0 MODE:ADC_LP
ADC1 ChMap:SWRM_TX2_CH1
TX SMIC MUX1:ZERO
TX_CDC_DMA_TX_3 Channels:One
TX_AIF1_CAP Mixer DEC1:0
ADC1_MIXER Switch:1
ADC1 Volume:6
MultiMedia1 Mixer TX_CDC_DMA_TX_3:0
TX_CDC_DMA_TX_3 SampleRate:KHZ_48

#capture_top-mic
#enable_top-mic
enable
TX_CDC_DMA_TX_3 Channels:One

TX DEC3 MUX:SWR_MIC
TX SMIC MUX3:SWR_MIC9
TX_AIF1_CAP Mixer DEC3:1
ADC4 ChMap:SWRM_TX3_CH2
ADC4 MUX:INP5
TX3 MODE:ADC_LP
ADC4_MIXER Switch:1
ADC4 Volume:8
MultiMedia1 Mixer TX_CDC_DMA_TX_3:1
TX_CDC_DMA_TX_3 SampleRate:$rate

#disable_top-mic
disable
TX SMIC MUX3:ZERO
TX_AIF1_CAP Mixer DEC3:0
ADC4 ChMap:SWRM_TX3_CH2
TX3 MODE:ADC_LP
TX_CDC_DMA_TX_3 Channels:One
ADC4_MIXER Switch:1
ADC4 Volume:6
MultiMedia1 Mixer TX_CDC_DMA_TX_3:0
TX_CDC_DMA_TX_3 SampleRate:KHZ_48

#capture_us
enable
Audio Stream Capture 0 App Type Cfg:69938 19 96000 196
TX_AIF2_CAP Mixer DEC2:1
TX DEC2 MUX:SWR_MIC
TX SMIC MUX2:SWR_MIC8
ADC3 ChMap:SWRM_TX3_CH1
HDR34 MUX:HDR34
ADC3_MIXER Switch:1
TX2 MODE:ADC_LP
ADC3 Volume:8
TX_DEC2 Volume:84
TX_CDC_DMA_TX_4 Channels:One
MultiMedia1 Mixer TX_CDC_DMA_TX_4:1
TX_CDC_DMA_TX_4 SampleRate:$rate

disable
ADC2 ChMap:ZERO
ADC3 ChMap:ZERO
ADC4 ChMap:SWRM_TX3_CH2
TX_AIF2_CAP Mixer DEC2:0
TX DEC2 MUX:SWR_MIC
TX SMIC MUX2:ZERO
HDR34 MUX:NO_HDR34
ADC3_MIXER Switch:0
TX2 MODE:ADC_LP

TX_DEC2 Volume:84
TX_CDC_DMA_TX_4 Channels:One
MultiMedia1 Mixer TX_CDC_DMA_TX_4:0
TX_CDC_DMA_TX_4 SampleRate:KHZ_96


#setup_mainmic2headphone
enable
TX0 MODE:ADC_LP
ADC1_MIXER Switch:1
ADC1 ChMap:SWRM_TX2_CH1
TX SMIC MUX0:SWR_MIC4
TX DEC0 MUX:SWR_MIC
RX INT0_1 MIX1 INP0:DEC0
RX INT1_1 MIX1 INP0:DEC0
RX INT0 DEM MUX:CLSH_DSM_OUT
RX INT1 DEM MUX:CLSH_DSM_OUT
RX_HPH_PWR_MODE:LOHIFI
RX HPH Mode:CLS_H_LOHIFI
RX_COMP1 Switch:0
RX_COMP2 Switch:0
HPHL_COMP Switch:0
HPHR_COMP Switch:0
RDAC3_MUX:RX1
HPHL_RDAC Switch:1
HPHR_RDAC Switch:1
ADC1 Volume:8
HPHL Volume:20
HPHR Volume:20
disable

#setup_headsetmic2headphone
enable
ADC2 MUX:INP2
HDR12 MUX:NO_HDR12
TX1 MODE:ADC_LP
ADC2_MIXER Switch:1
ADC2 ChMap:SWRM_TX2_CH2
TX SMIC MUX0:SWR_MIC5
TX DEC0 MUX:SWR_MIC
RX INT0_1 MIX1 INP0:DEC0
RX INT1_1 MIX1 INP0:DEC0
RX INT0 DEM MUX:CLSH_DSM_OUT
RX INT1 DEM MUX:CLSH_DSM_OUT
RX_HPH_PWR_MODE:LOHIFI
RX HPH Mode:CLS_H_LOHIFI
RX_COMP1 Switch:0
RX_COMP2 Switch:0
HPHL_COMP Switch:0
HPHR_COMP Switch:0
RDAC3_MUX:RX1
HPHL_RDAC Switch:1
HPHR_RDAC Switch:1
HPHL Volume:20
HPHR Volume:20
disable

#setup_topmic2headphone
enable
ADC4 MUX:INP5
TX3 MODE:ADC_LP
ADC4_MIXER Switch:1
ADC4 ChMap:SWRM_TX3_CH2
TX SMIC MUX0:SWR_MIC9
TX DEC0 MUX:SWR_MIC
RX INT0_1 MIX1 INP0:DEC0
RX INT1_1 MIX1 INP0:DEC0
RX INT0 DEM MUX:CLSH_DSM_OUT
RX INT1 DEM MUX:CLSH_DSM_OUT
RX_HPH_PWR_MODE:LOHIFI
RX HPH Mode:CLS_H_LOHIFI
RX_COMP1 Switch:0
RX_COMP2 Switch:0
HPHL_COMP Switch:0
HPHR_COMP Switch:0
RDAC3_MUX:RX1
HPHL_RDAC Switch:1
HPHR_RDAC Switch:1
ADC4 Volume:8
HPHL Volume:20
HPHR Volume:20
disable

#teardown_loopback
enable
HPHR_RDAC Switch:0
HPHL_RDAC Switch:0
RDAC3_MUX:RX1
HPHR_COMP Switch:0
HPHL_COMP Switch:0
RX_COMP2 Switch:0
RX_COMP1 Switch:0
RX HPH Mode:CLS_H_ULP
RX_HPH_PWR_MODE:ULP
RX INT1 DEM MUX:NORMAL_DSM_OUT
RX INT0 DEM MUX:NORMAL_DSM_OUT
RX INT1_1 MIX1 INP0:ZERO
RX INT0_1 MIX1 INP0:ZERO
TX DEC0 MUX:ZERO
TX SMIC MUX0:ZERO
ADC1 ChMap:SWRM_TX2_CH1
ADC2 ChMap:ZERO
ADC3 ChMap:ZERO
ADC4 ChMap:SWRM_TX3_CH2
ADC1_MIXER Switch:1
ADC2_MIXER Switch:0
ADC3_MIXER Switch:0
ADC4_MIXER Switch:1
TX0 MODE:ADC_LP
TX2 MODE:ADC_LP
TX3 MODE:ADC_LP
HDR12 MUX:NO_HDR12
ADC2 MUX:INP2
ADC4 MUX:INP5
HPHL Volume:20
HPHR Volume:20
ADC1 Volume:6
ADC2 Volume:6
ADC3 Volume:6
ADC4 Volume:6
disable
