WDCTL(8)

NAME
wdctl - show hardware watchdog status

SYNOPSIS

wdctl [options] [device...]

DESCRIPTION

Show hardware watchdog status. The default device is /dev/watchdog. If more than one device is specified then the output is separated by one blank line.

If the device is already used or user has no permissions to read from the device, then wdctl reads data from sysfs. In this case information about supported features (flags) might be missing.

Note that the number of supported watchdog features is hardware specific.

OPTIONS

-f, --flags list
    Print only the specified flags.

-F, --noflags
    Do not print information about flags.

-I, --noident
    Do not print watchdog identity information.

-n, --noheadings
    Do not print a header line for flags table.

-o, --output list
    Define the output columns to use in table of watchdog flags. If no output arrangement is specified, then a default set is used. Use --help to get list of all supported columns.

-O, --oneline
    Print all wanted information on one line in key="value" output format.

-r, --raw
    Use the raw output format.

-s, -settimeout seconds
    Set the watchdog timeout in seconds.

-T, --notimeouts
    Do not print watchdog timeouts.

-x, --flags-only
    Same as -I -T.

-V, --version
    Display version information and exit.

-h, --help
    Display help text and exit.

AUTHORS

REPORTING BUGS

For bug reports, use the issue tracker at

AVAILABILITY

The wdctl command is part of the util-linux package which can be downloaded from