SETKEYCODES(8)

NAME
setkeycodes - load kernel scancode-to-keycode mapping table entries

SYNOPSIS
setkeycodes scancode keycode ...

DESCRIPTION
The setkeycodes command reads its arguments two at a time, each pair of arguments consisting of a scancode (given in hexadecimal) and a keycode (given in decimal). For each such pair, it tells the kernel keyboard driver to map the specified scancode to the specified keycode. This command is useful only for people with slightly unusual keyboards, that have a few keys which produce scancodes that the kernel does not recognize.

THEORY
The usual PC keyboard produces a series of scancodes for each key press and key release. (Scancodes are shown by showkey -s, see showkey(1) ) The kernel parses this stream of scancodes, and converts it to a stream of keycodes (key press/release events). (Keycodes are shown by showkey.) Apart from a few scancodes with special meaning, and apart from the sequence produced by the Pause key, and apart from shiftstate related scancodes, and apart from the key up/down bit, the stream of scancodes consists of unescaped scancodes xx (7 bits) and escaped scancodes e0 xx (8+7 bits). To these scancodes or scancode pairs, a corresponding keycode can be assigned (in the range 1-127). For example, if you have a Macro key that produces e0 6f according to showkey(1), the command
    setkeycodes e06f 112
will assign the keycode 112 to it, and then loadkeys(1) can be used to define the function of this key. USB keyboards have standardized keycodes and setkeycodes doesn't affect them at all.

Some older kernels might hardwire a low scancode range to the equivalent keycodes; setkeycodes will fail when you try to remap these.

2.6 KERNELS
In 2.6 kernels key codes lie in the range 1-255, instead of 1-127. (It might be best to confine oneself to the range 1-239.)

In 2.6 kernels raw mode, or scancode mode, is not very raw at all. The code returned by showkey -s will change after use of setkeycodes. A kernel bug. See also showkey(1).

OPTIONS
None.

BUGS
The keycodes of X have nothing to do with those of Linux. Unusual keys can be made visible under Linux, but not under X. setkeycodes affects only the "first" input device that has modifiable scancode-to-keycode mapping. If there is more than one such device, setkeycodes cannot change the mapping of other devices than the "first" one.

SEE ALSO
dumpkeys(1), loadkeys(1), showkey(1), getkeycodes(8)