Connmark retriever action in tc(8)

NAME
connmark - netfilter connmark retriever action

SYNOPSIS
tc ... action connmark [ zone u16_zone_index ] [ CONTROL ] [ index u32_index ]
CONTROL := { reclassify | pipe | drop | continue | ok }

DESCRIPTION
The connmark action is used to restore the connection's mark value into the packet's fwmark.

OPTIONS

zone u16_zone_index
    Specify the conntrack zone when doing conntrack lookups for packets. u16_zone_index is a 16bit unsigned decimal value.

CONTROL
    How to continue after executing this action.

    reclassify
        Restarts classification by jumping back to the first filter attached to this action's parent.

    pipe
        Continue with the next action, this is the default.

    drop
    shot
        Packet will be dropped without running further actions.

    continue
        Continue classification with next filter in line.

    pass
        Return to calling qdisc for packet processing. This ends the classification process.

index u32_index
    Specify an index for this action in order to being able to identify it in later commands. u32_index is a 32bit unsigned decimal value.

SEE ALSO
tc(8)